<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.1.0">
<drawing>
<schematic>
<libraries>
<library name="FRAMES">
<packages>
</packages>
<symbols>
<symbol name="DINA4_L">
</symbol>
<symbol name="DOCFIELD">
</symbol>
</symbols>
<devicesets>
<deviceset name="DINA4_L" prefix="FRAME" uservalue="yes">
<description>&lt;b&gt;FRAME&lt;/b&gt;&lt;p&gt;
DIN A4, landscape with extra doc field</description>
<gates>
<gate name="G$1" symbol="DINA4_L"/>
<gate name="G$2" symbol="DOCFIELD"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
<library name="supply1">
<packages>
</packages>
<symbols>
<symbol name="+5V">
<pin name="+5V" direction="sup"/>
</symbol>
<symbol name="GND">
<pin name="GND" direction="sup"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="+5V" prefix="P+">
<description>&lt;b&gt;SUPPLY SYMBOL&lt;/b&gt;</description>
<gates>
<gate name="1" symbol="+5V"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="GND" prefix="GND">
<description>&lt;b&gt;SUPPLY SYMBOL&lt;/b&gt;</description>
<gates>
<gate name="1" symbol="GND"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
<library name="1Eigene">
<packages>
<package name="SW-PUSH-90">
</package>
<package name="ESP201">
</package>
<package name="207.10">
</package>
<package name="SOT23">
<description>&lt;b&gt;SMALL OUTLINE TRANSISTOR&lt;/b&gt;&lt;p&gt;
reflow soldering</description>
</package>
</packages>
<symbols>
<symbol name="SW-PUSH-90">
<pin name="P1" direction="pas"/>
<pin name="S1" direction="pas"/>
<pin name="G2" direction="pas"/>
<pin name="G1" direction="pas"/>
</symbol>
<symbol name="ESP201">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="C" direction="pas"/>
</symbol>
<symbol name="WIDERSTAND">
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
</symbol>
<symbol name="LM809">
<pin name="GND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="/RESET" direction="out"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="SW-PUSH-90" prefix="SW">
<gates>
<gate name="G$1" symbol="SW-PUSH-90"/>
</gates>
<devices>
<device name="" package="SW-PUSH-90">
<connects>
<connect gate="G$1" pin="G1" pad="3"/>
<connect gate="G$1" pin="G2" pad="4"/>
<connect gate="G$1" pin="P1" pad="1"/>
<connect gate="G$1" pin="S1" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ESP201" prefix="SW">
<gates>
<gate name="G$1" symbol="ESP201"/>
</gates>
<devices>
<device name="" package="ESP201">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WIDERSTAND_10" prefix="R" uservalue="yes">
<gates>
<gate name="G$1" symbol="WIDERSTAND"/>
</gates>
<devices>
<device name="" package="207.10">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM809M3-4.63" prefix="IC">
<gates>
<gate name="G$1" symbol="LM809"/>
</gates>
<devices>
<device name="" package="SOT23">
<connects>
<connect gate="G$1" pin="/RESET" pad="2"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="VCC" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
<library name="rcl">
<packages>
<package name="C0402">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;</description>
</package>
<package name="C0504">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;</description>
</package>
<package name="C0603">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;</description>
</package>
<package name="C0805">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;</description>
</package>
<package name="C1005">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;</description>
</package>
<package name="C1206">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;</description>
</package>
<package name="C1210">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;</description>
</package>
<package name="C1310">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;</description>
</package>
<package name="C1608">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;</description>
</package>
<package name="C1812">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;</description>
</package>
<package name="C1825">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;</description>
</package>
<package name="C2012">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;</description>
</package>
<package name="C3216">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;</description>
</package>
<package name="C3225">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;</description>
</package>
<package name="C4532">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;</description>
</package>
<package name="C4564">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;</description>
</package>
<package name="C025-024X044">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 2.5 mm, outline 2.4 x 4.4 mm</description>
</package>
<package name="C025-025X050">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 2.5 mm, outline 2.5 x 5 mm</description>
</package>
<package name="C025-030X050">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 2.5 mm, outline 3 x 5 mm</description>
</package>
<package name="C025-040X050">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 2.5 mm, outline 4 x 5 mm</description>
</package>
<package name="C025-050X050">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 2.5 mm, outline 5 x 5 mm</description>
</package>
<package name="C025-060X050">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 2.5 mm, outline 6 x 5 mm</description>
</package>
<package name="C025_050-024X070">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 2.5 mm + 5 mm, outline 2.4 x 7 mm</description>
</package>
<package name="C025_050-025X075">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 2.5 + 5 mm, outline 2.5 x 7.5 mm</description>
</package>
<package name="C025_050-035X075">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 2.5 + 5 mm, outline 3.5 x 7.5 mm</description>
</package>
<package name="C025_050-045X075">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 2.5 + 5 mm, outline 4.5 x 7.5 mm</description>
</package>
<package name="C025_050-055X075">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 2.5 + 5 mm, outline 5.5 x 7.5 mm</description>
</package>
<package name="C050-024X044">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 5 mm, outline 2.4 x 4.4 mm</description>
</package>
<package name="C050-025X075">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 5 mm, outline 2.5 x 7.5 mm</description>
</package>
<package name="C050-045X075">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 5 mm, outline 4.5 x 7.5 mm</description>
</package>
<package name="C050-030X075">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 5 mm, outline 3 x 7.5 mm</description>
</package>
<package name="C050-050X075">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 5 mm, outline 5 x 7.5 mm</description>
</package>
<package name="C050-055X075">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 5 mm, outline 5.5 x 7.5 mm</description>
</package>
<package name="C050-075X075">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 5 mm, outline 7.5 x 7.5 mm</description>
</package>
<package name="C050H075X075">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
Horizontal, grid 5 mm, outline 7.5 x 7.5 mm</description>
</package>
<package name="C075-032X103">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 7.5 mm, outline 3.2 x 10.3 mm</description>
</package>
<package name="C075-042X103">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 7.5 mm, outline 4.2 x 10.3 mm</description>
</package>
<package name="C075-052X106">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 7.5 mm, outline 5.2 x 10.6 mm</description>
</package>
<package name="C102-043X133">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 10.2 mm, outline 4.3 x 13.3 mm</description>
</package>
<package name="C102-054X133">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 10.2 mm, outline 5.4 x 13.3 mm</description>
</package>
<package name="C102-064X133">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 10.2 mm, outline 6.4 x 13.3 mm</description>
</package>
<package name="C102_152-062X184">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 10.2 mm + 15.2 mm, outline 6.2 x 18.4 mm</description>
</package>
<package name="C150-054X183">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 15 mm, outline 5.4 x 18.3 mm</description>
</package>
<package name="C150-064X183">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 15 mm, outline 6.4 x 18.3 mm</description>
</package>
<package name="C150-072X183">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 15 mm, outline 7.2 x 18.3 mm</description>
</package>
<package name="C150-084X183">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 15 mm, outline 8.4 x 18.3 mm</description>
</package>
<package name="C150-091X182">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 15 mm, outline 9.1 x 18.2 mm</description>
</package>
<package name="C225-062X268">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 22.5 mm, outline 6.2 x 26.8 mm</description>
</package>
<package name="C225-074X268">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 22.5 mm, outline 7.4 x 26.8 mm</description>
</package>
<package name="C225-087X268">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 22.5 mm, outline 8.7 x 26.8 mm</description>
</package>
<package name="C225-108X268">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 22.5 mm, outline 10.8 x 26.8 mm</description>
</package>
<package name="C225-113X268">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 22.5 mm, outline 11.3 x 26.8 mm</description>
</package>
<package name="C275-093X316">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 27.5 mm, outline 9.3 x 31.6 mm</description>
</package>
<package name="C275-113X316">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 27.5 mm, outline 11.3 x 31.6 mm</description>
</package>
<package name="C275-134X316">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 27.5 mm, outline 13.4 x 31.6 mm</description>
</package>
<package name="C275-205X316">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 27.5 mm, outline 20.5 x 31.6 mm</description>
</package>
<package name="C325-137X374">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 32.5 mm, outline 13.7 x 37.4 mm</description>
</package>
<package name="C325-162X374">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 32.5 mm, outline 16.2 x 37.4 mm</description>
</package>
<package name="C325-182X374">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 32.5 mm, outline 18.2 x 37.4 mm</description>
</package>
<package name="C375-192X418">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 37.5 mm, outline 19.2 x 41.8 mm</description>
</package>
<package name="C375-203X418">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 37.5 mm, outline 20.3 x 41.8 mm</description>
</package>
<package name="C050-035X075">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 5 mm, outline 3.5 x 7.5 mm</description>
</package>
<package name="C375-155X418">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 37.5 mm, outline 15.5 x 41.8 mm</description>
</package>
<package name="C075-063X106">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 7.5 mm, outline 6.3 x 10.6 mm</description>
</package>
<package name="C275-154X316">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 27.5 mm, outline 15.4 x 31.6 mm</description>
</package>
<package name="C275-173X316">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 27.5 mm, outline 17.3 x 31.6 mm</description>
</package>
<package name="C0402K">
<description>&lt;b&gt;Ceramic Chip Capacitor KEMET 0204 reflow solder&lt;/b&gt;&lt;p&gt;
Metric Code Size 1005</description>
</package>
<package name="C0603K">
<description>&lt;b&gt;Ceramic Chip Capacitor KEMET 0603 reflow solder&lt;/b&gt;&lt;p&gt;
Metric Code Size 1608</description>
</package>
<package name="C0805K">
<description>&lt;b&gt;Ceramic Chip Capacitor KEMET 0805 reflow solder&lt;/b&gt;&lt;p&gt;
Metric Code Size 2012</description>
</package>
<package name="C1206K">
<description>&lt;b&gt;Ceramic Chip Capacitor KEMET 1206 reflow solder&lt;/b&gt;&lt;p&gt;
Metric Code Size 3216</description>
</package>
<package name="C1210K">
<description>&lt;b&gt;Ceramic Chip Capacitor KEMET 1210 reflow solder&lt;/b&gt;&lt;p&gt;
Metric Code Size 3225</description>
</package>
<package name="C1812K">
<description>&lt;b&gt;Ceramic Chip Capacitor KEMET 1812 reflow solder&lt;/b&gt;&lt;p&gt;
Metric Code Size 4532</description>
</package>
<package name="C1825K">
<description>&lt;b&gt;Ceramic Chip Capacitor KEMET 1825 reflow solder&lt;/b&gt;&lt;p&gt;
Metric Code Size 4564</description>
</package>
<package name="C2220K">
<description>&lt;b&gt;Ceramic Chip Capacitor KEMET 2220 reflow solder&lt;/b&gt;&lt;p&gt;Metric Code Size 5650</description>
</package>
<package name="C2225K">
<description>&lt;b&gt;Ceramic Chip Capacitor KEMET 2225 reflow solder&lt;/b&gt;&lt;p&gt;Metric Code Size 5664</description>
</package>
<package name="HPC0201">
<description>&lt;b&gt; &lt;/b&gt;&lt;p&gt;
Source: http://www.vishay.com/docs/10129/hpc0201a.pdf</description>
</package>
<package name="C0201">
<description>Source: http://www.avxcorp.com/docs/catalogs/cx5r.pdf</description>
</package>
<package name="R0402">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;</description>
</package>
<package name="R0603">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;</description>
</package>
<package name="R0805">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;</description>
</package>
<package name="R0805W">
<description>&lt;b&gt;RESISTOR&lt;/b&gt; wave soldering&lt;p&gt;</description>
</package>
<package name="R1005">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;</description>
</package>
<package name="R1206">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;</description>
</package>
<package name="R1206W">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
wave soldering</description>
</package>
<package name="R1210">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;</description>
</package>
<package name="R1210W">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
wave soldering</description>
</package>
<package name="R2010">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;</description>
</package>
<package name="R2010W">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
wave soldering</description>
</package>
<package name="R2012">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;</description>
</package>
<package name="R2012W">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
wave soldering</description>
</package>
<package name="R2512">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;</description>
</package>
<package name="R2512W">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
wave soldering</description>
</package>
<package name="R3216">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;</description>
</package>
<package name="R3216W">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
wave soldering</description>
</package>
<package name="R3225">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;</description>
</package>
<package name="R3225W">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
wave soldering</description>
</package>
<package name="R5025">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;</description>
</package>
<package name="R5025W">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
wave soldering</description>
</package>
<package name="R6332">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
Source: http://download.siliconexpert.com/pdfs/2005/02/24/Semi_Ap/2/VSH/Resistor/dcrcwfre.pdf</description>
</package>
<package name="R6332W">
<description>&lt;b&gt;RESISTOR&lt;/b&gt; wave soldering&lt;p&gt;
Source: http://download.siliconexpert.com/pdfs/2005/02/24/Semi_Ap/2/VSH/Resistor/dcrcwfre.pdf</description>
</package>
<package name="M0805">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
MELF 0.10 W</description>
</package>
<package name="M1206">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
MELF 0.25 W</description>
</package>
<package name="M1406">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
MELF 0.12 W</description>
</package>
<package name="M2012">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
MELF 0.10 W</description>
</package>
<package name="M2309">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
MELF 0.25 W</description>
</package>
<package name="M3216">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
MELF 0.25 W</description>
</package>
<package name="M3516">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
MELF 0.12 W</description>
</package>
<package name="M5923">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
MELF 0.25 W</description>
</package>
<package name="0207/10">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0207, grid 10 mm</description>
</package>
<package name="0207/12">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0207, grid 12 mm</description>
</package>
<package name="0207/15">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0207, grid 15mm</description>
</package>
<package name="0207/2V">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0207, grid 2.5 mm</description>
</package>
<package name="0207/5V">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0207, grid 5 mm</description>
</package>
<package name="0207/7">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0207, grid 7.5 mm</description>
</package>
<package name="0309/10">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0309, grid 10mm</description>
</package>
<package name="0309/12">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0309, grid 12.5 mm</description>
</package>
<package name="0309V">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0309, grid 2.5 mm</description>
</package>
<package name="0411/12">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0411, grid 12.5 mm</description>
</package>
<package name="0411/15">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0411, grid 15 mm</description>
</package>
<package name="0414/15">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0414, grid 15 mm</description>
</package>
<package name="0414V">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0414, grid 5 mm</description>
</package>
<package name="0617/17">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0617, grid 17.5 mm</description>
</package>
<package name="0617V">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0617, grid 5 mm</description>
</package>
<package name="0922/22">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0922, grid 22.5 mm</description>
</package>
<package name="P0613V">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0613, grid 5 mm</description>
</package>
<package name="P0613/15">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0613, grid 15 mm</description>
</package>
<package name="P0817/22">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0817, grid 22.5 mm</description>
</package>
<package name="P0817V">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0817, grid 6.35 mm</description>
</package>
<package name="V234/12">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type V234, grid 12.5 mm</description>
</package>
<package name="V235/17">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type V235, grid 17.78 mm</description>
</package>
<package name="V526-0">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type V526-0, grid 2.5 mm</description>
</package>
<package name="MINI_MELF-0102R">
<description>&lt;b&gt;CECC Size RC2211&lt;/b&gt; Reflow Soldering&lt;p&gt;
source Beyschlag</description>
</package>
<package name="MINI_MELF-0102W">
<description>&lt;b&gt;CECC Size RC2211&lt;/b&gt; Wave Soldering&lt;p&gt;
source Beyschlag</description>
</package>
<package name="MINI_MELF-0204R">
<description>&lt;b&gt;CECC Size RC3715&lt;/b&gt; Reflow Soldering&lt;p&gt;
source Beyschlag</description>
</package>
<package name="MINI_MELF-0204W">
<description>&lt;b&gt;CECC Size RC3715&lt;/b&gt; Wave Soldering&lt;p&gt;
source Beyschlag</description>
</package>
<package name="MINI_MELF-0207R">
<description>&lt;b&gt;CECC Size RC6123&lt;/b&gt; Reflow Soldering&lt;p&gt;
source Beyschlag</description>
</package>
<package name="MINI_MELF-0207W">
<description>&lt;b&gt;CECC Size RC6123&lt;/b&gt; Wave Soldering&lt;p&gt;
source Beyschlag</description>
</package>
<package name="0922V">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0922, grid 7.5 mm</description>
</package>
<package name="RDH/15">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type RDH, grid 15 mm</description>
</package>
<package name="MINI_MELF-0102AX">
<description>&lt;b&gt;Mini MELF 0102 Axial&lt;/b&gt;</description>
</package>
<package name="R0201">
<description>&lt;b&gt;RESISTOR&lt;/b&gt; chip&lt;p&gt;
Source: http://www.vishay.com/docs/20008/dcrcw.pdf</description>
</package>
<package name="VTA52">
<description>&lt;b&gt;Bulk Metal® Foil Technology&lt;/b&gt;, Tubular Axial Lead Resistors, Meets or Exceeds MIL-R-39005 Requirements&lt;p&gt;
MIL SIZE RBR52&lt;br&gt;
Source: VISHAY .. vta56.pdf</description>
</package>
<package name="VTA53">
<description>&lt;b&gt;Bulk Metal® Foil Technology&lt;/b&gt;, Tubular Axial Lead Resistors, Meets or Exceeds MIL-R-39005 Requirements&lt;p&gt;
MIL SIZE RBR53&lt;br&gt;
Source: VISHAY .. vta56.pdf</description>
</package>
<package name="VTA54">
<description>&lt;b&gt;Bulk Metal® Foil Technology&lt;/b&gt;, Tubular Axial Lead Resistors, Meets or Exceeds MIL-R-39005 Requirements&lt;p&gt;
MIL SIZE RBR54&lt;br&gt;
Source: VISHAY .. vta56.pdf</description>
</package>
<package name="VTA55">
<description>&lt;b&gt;Bulk Metal® Foil Technology&lt;/b&gt;, Tubular Axial Lead Resistors, Meets or Exceeds MIL-R-39005 Requirements&lt;p&gt;
MIL SIZE RBR55&lt;br&gt;
Source: VISHAY .. vta56.pdf</description>
</package>
<package name="VTA56">
<description>&lt;b&gt;Bulk Metal® Foil Technology&lt;/b&gt;, Tubular Axial Lead Resistors, Meets or Exceeds MIL-R-39005 Requirements&lt;p&gt;
MIL SIZE RBR56&lt;br&gt;
Source: VISHAY .. vta56.pdf</description>
</package>
<package name="VMTA55">
<description>&lt;b&gt;Bulk Metal® Foil Technology&lt;/b&gt;, Tubular Axial Lead Resistors, Meets or Exceeds MIL-R-39005 Requirements&lt;p&gt;
MIL SIZE RNC55&lt;br&gt;
Source: VISHAY .. vta56.pdf</description>
</package>
<package name="VMTB60">
<description>&lt;b&gt;Bulk Metal® Foil Technology&lt;/b&gt;, Tubular Axial Lead Resistors, Meets or Exceeds MIL-R-39005 Requirements&lt;p&gt;
MIL SIZE RNC60&lt;br&gt;
Source: VISHAY .. vta56.pdf</description>
</package>
<package name="R4527">
<description>&lt;b&gt;Package 4527&lt;/b&gt;&lt;p&gt;
Source: http://www.vishay.com/docs/31059/wsrhigh.pdf</description>
</package>
<package name="WSC0001">
<description>&lt;b&gt;Wirewound Resistors, Precision Power&lt;/b&gt;&lt;p&gt;
Source: VISHAY wscwsn.pdf</description>
</package>
<package name="WSC0002">
<description>&lt;b&gt;Wirewound Resistors, Precision Power&lt;/b&gt;&lt;p&gt;
Source: VISHAY wscwsn.pdf</description>
</package>
<package name="WSC01/2">
<description>&lt;b&gt;Wirewound Resistors, Precision Power&lt;/b&gt;&lt;p&gt;
Source: VISHAY wscwsn.pdf</description>
</package>
<package name="WSC2515">
<description>&lt;b&gt;Wirewound Resistors, Precision Power&lt;/b&gt;&lt;p&gt;
Source: VISHAY wscwsn.pdf</description>
</package>
<package name="WSC4527">
<description>&lt;b&gt;Wirewound Resistors, Precision Power&lt;/b&gt;&lt;p&gt;
Source: VISHAY wscwsn.pdf</description>
</package>
<package name="WSC6927">
<description>&lt;b&gt;Wirewound Resistors, Precision Power&lt;/b&gt;&lt;p&gt;
Source: VISHAY wscwsn.pdf</description>
</package>
<package name="R1218">
<description>&lt;b&gt;CRCW1218 Thick Film, Rectangular Chip Resistors&lt;/b&gt;&lt;p&gt;
Source: http://www.vishay.com .. dcrcw.pdf</description>
</package>
<package name="0204/5">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0204, grid 5 mm</description>
</package>
<package name="0204/7">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0204, grid 7.5 mm</description>
</package>
<package name="0204V">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0204, grid 2.5 mm</description>
</package>
<package name="0411V">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0411, grid 3.81 mm</description>
</package>
<package name="0617/22">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0617, grid 22.5 mm</description>
</package>
</packages>
<symbols>
<symbol name="C-EU">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="R-EU">
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="C-EU" prefix="C" uservalue="yes">
<description>&lt;B&gt;CAPACITOR&lt;/B&gt;, European symbol</description>
<gates>
<gate name="G$1" symbol="C-EU"/>
</gates>
<devices>
<device name="C0402" package="C0402">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C0504" package="C0504">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C0603" package="C0603">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C0805" package="C0805">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C1005" package="C1005">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C1206" package="C1206">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C1210" package="C1210">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C1310" package="C1310">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C1608" package="C1608">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C1812" package="C1812">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C1825" package="C1825">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C2012" package="C2012">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C3216" package="C3216">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C3225" package="C3225">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C4532" package="C4532">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C4564" package="C4564">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="025-024X044" package="C025-024X044">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="025-025X050" package="C025-025X050">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="025-030X050" package="C025-030X050">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="025-040X050" package="C025-040X050">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="025-050X050" package="C025-050X050">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="025-060X050" package="C025-060X050">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C025_050-024X070" package="C025_050-024X070">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="025_050-025X075" package="C025_050-025X075">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="025_050-035X075" package="C025_050-035X075">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="025_050-045X075" package="C025_050-045X075">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="025_050-055X075" package="C025_050-055X075">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="050-024X044" package="C050-024X044">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="050-025X075" package="C050-025X075">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="050-045X075" package="C050-045X075">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="050-030X075" package="C050-030X075">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="050-050X075" package="C050-050X075">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="050-055X075" package="C050-055X075">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="050-075X075" package="C050-075X075">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="050H075X075" package="C050H075X075">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="075-032X103" package="C075-032X103">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="075-042X103" package="C075-042X103">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="075-052X106" package="C075-052X106">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="102-043X133" package="C102-043X133">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="102-054X133" package="C102-054X133">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="102-064X133" package="C102-064X133">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="102_152-062X184" package="C102_152-062X184">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="150-054X183" package="C150-054X183">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="150-064X183" package="C150-064X183">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="150-072X183" package="C150-072X183">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="150-084X183" package="C150-084X183">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="150-091X182" package="C150-091X182">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="225-062X268" package="C225-062X268">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="225-074X268" package="C225-074X268">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="225-087X268" package="C225-087X268">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="225-108X268" package="C225-108X268">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="225-113X268" package="C225-113X268">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="275-093X316" package="C275-093X316">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="275-113X316" package="C275-113X316">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="275-134X316" package="C275-134X316">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="275-205X316" package="C275-205X316">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="325-137X374" package="C325-137X374">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="325-162X374" package="C325-162X374">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="325-182X374" package="C325-182X374">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="375-192X418" package="C375-192X418">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="375-203X418" package="C375-203X418">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="050-035X075" package="C050-035X075">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="375-155X418" package="C375-155X418">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="075-063X106" package="C075-063X106">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="275-154X316" package="C275-154X316">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="275-173X316" package="C275-173X316">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C0402K" package="C0402K">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C0603K" package="C0603K">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C0805K" package="C0805K">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C1206K" package="C1206K">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C1210K" package="C1210K">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C1812K" package="C1812K">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C1825K" package="C1825K">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C2220K" package="C2220K">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C2225K" package="C2225K">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="HPC0201" package="HPC0201">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C0201" package="C0201">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="R-EU_" prefix="R" uservalue="yes">
<description>&lt;B&gt;RESISTOR&lt;/B&gt;, European symbol</description>
<gates>
<gate name="G$1" symbol="R-EU"/>
</gates>
<devices>
<device name="R0402" package="R0402">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="R0603" package="R0603">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="R0805" package="R0805">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="R0805W" package="R0805W">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="R1005" package="R1005">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="R1206" package="R1206">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="R1206W" package="R1206W">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="R1210" package="R1210">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="R1210W" package="R1210W">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="R2010" package="R2010">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="R2010W" package="R2010W">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="R2012" package="R2012">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="R2012W" package="R2012W">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="R2512" package="R2512">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="R2512W" package="R2512W">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="R3216" package="R3216">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="R3216W" package="R3216W">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="R3225" package="R3225">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="R3225W" package="R3225W">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="R5025" package="R5025">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="R5025W" package="R5025W">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="R6332" package="R6332">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="R6332W" package="R6332W">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="M0805" package="M0805">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="M1206" package="M1206">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="M1406" package="M1406">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="M2012" package="M2012">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="M2309" package="M2309">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="M3216" package="M3216">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="M3516" package="M3516">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="M5923" package="M5923">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0204/5" package="0204/5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0204/7" package="0204/7">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0204/2V" package="0204V">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0207/10" package="0207/10">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0207/12" package="0207/12">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0207/15" package="0207/15">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0207/2V" package="0207/2V">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0207/5V" package="0207/5V">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0207/7" package="0207/7">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0309/10" package="0309/10">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0309/12" package="0309/12">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0309/V" package="0309V">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0411/12" package="0411/12">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0411/15" package="0411/15">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0411/3V" package="0411V">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0414/15" package="0414/15">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0414/5V" package="0414V">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0617/17" package="0617/17">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0617/22" package="0617/22">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0617/5V" package="0617V">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0922/22" package="0922/22">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0613/5V" package="P0613V">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0613/15" package="P0613/15">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0817/22" package="P0817/22">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0817/7V" package="P0817V">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="V234/12" package="V234/12">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="V235/17" package="V235/17">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="V526-0" package="V526-0">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="MELF0102R" package="MINI_MELF-0102R">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="MELF0102W" package="MINI_MELF-0102W">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="MELF0204R" package="MINI_MELF-0204R">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="MELF0204W" package="MINI_MELF-0204W">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="MELF0207R" package="MINI_MELF-0207R">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="MELF0207W" package="MINI_MELF-0207W">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0922V" package="0922V">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="RDH/15" package="RDH/15">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="MELF0102AX" package="MINI_MELF-0102AX">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="R0201" package="R0201">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="VTA52" package="VTA52">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="VTA53" package="VTA53">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="VTA54" package="VTA54">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="VTA55" package="VTA55">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="VTA56" package="VTA56">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="VMTA55" package="VMTA55">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="VMTB60" package="VMTB60">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="R4527" package="R4527">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="WSC0001" package="WSC0001">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="WSC0002" package="WSC0002">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="WSC01/2" package="WSC01/2">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="WSC2515" package="WSC2515">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="WSC4527" package="WSC4527">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="WSC6927" package="WSC6927">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="R1218" package="R1218">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
<library name="transistor-npn">
<packages>
<package name="TO92-EBC">
<description>&lt;b&gt;TO-92&lt;/b&gt;&lt;p&gt;
 grid 5.08 mm</description>
</package>
</packages>
<symbols>
<symbol name="NPN">
<pin name="B" direction="pas"/>
<pin name="E" direction="pas"/>
<pin name="C" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="BC546*" prefix="Q">
<description>&lt;b&gt;NPN Transistor&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="NPN"/>
</gates>
<devices>
<device name="" package="TO92-EBC">
<connects>
<connect gate="G$1" pin="B" pad="B"/>
<connect gate="G$1" pin="C" pad="C"/>
<connect gate="G$1" pin="E" pad="E"/>
</connects>
<technologies>
<technology name="A"/>
<technology name="B"/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
<library name="pinhead-2">
<packages>
<package name="2X21">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt; - 2.54</description>
</package>
<package name="2X21/90">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt; - 2.54 90°</description>
</package>
<package name="2X21M">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt; - 2</description>
</package>
<package name="2X21SMD">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt; - 2.54 SMD</description>
</package>
<package name="2X21SMD/90">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt; - 2.54 90°</description>
</package>
<package name="2X06">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt; - 2.54</description>
</package>
<package name="2X06/90">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt; - 2.54 90°</description>
</package>
<package name="2X06M">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt; - 2</description>
</package>
<package name="2X06SMD">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt; - 2.54 SMD</description>
</package>
<package name="MICROMATCH-12">
<description>&lt;b&gt;MicroMaTch 12 &lt;/b&gt; 8-215464-2 / 1-215464-2&lt;p&gt;
Drawing Number C-215464&lt;br&gt;
DDEController.pdf</description>
</package>
<package name="2X06SMD/90">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt; - 2.54 90°</description>
</package>
<package name="2X13">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt; - 2.54</description>
</package>
<package name="2X13/90">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt; - 2.54 90°</description>
</package>
<package name="2X13M">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt; - 2</description>
</package>
<package name="2X13SMD">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt; - 2.54 SMD</description>
</package>
<package name="2X13SMD/90">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt; - 2.54 90°</description>
</package>
</packages>
<symbols>
<symbol name="PINH2X21">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
<pin name="4" direction="pas" function="dot"/>
<pin name="5" direction="pas" function="dot"/>
<pin name="6" direction="pas" function="dot"/>
<pin name="7" direction="pas" function="dot"/>
<pin name="8" direction="pas" function="dot"/>
<pin name="9" direction="pas" function="dot"/>
<pin name="10" direction="pas" function="dot"/>
<pin name="11" direction="pas" function="dot"/>
<pin name="12" direction="pas" function="dot"/>
<pin name="13" direction="pas" function="dot"/>
<pin name="14" direction="pas" function="dot"/>
<pin name="15" direction="pas" function="dot"/>
<pin name="16" direction="pas" function="dot"/>
<pin name="17" direction="pas" function="dot"/>
<pin name="18" direction="pas" function="dot"/>
<pin name="19" direction="pas" function="dot"/>
<pin name="20" direction="pas" function="dot"/>
<pin name="21" direction="pas" function="dot"/>
<pin name="22" direction="pas" function="dot"/>
<pin name="23" direction="pas" function="dot"/>
<pin name="24" direction="pas" function="dot"/>
<pin name="25" direction="pas" function="dot"/>
<pin name="26" direction="pas" function="dot"/>
<pin name="27" direction="pas" function="dot"/>
<pin name="28" direction="pas" function="dot"/>
<pin name="29" direction="pas" function="dot"/>
<pin name="30" direction="pas" function="dot"/>
<pin name="31" direction="pas" function="dot"/>
<pin name="32" direction="pas" function="dot"/>
<pin name="33" direction="pas" function="dot"/>
<pin name="34" direction="pas" function="dot"/>
<pin name="35" direction="pas" function="dot"/>
<pin name="36" direction="pas" function="dot"/>
<pin name="37" direction="pas" function="dot"/>
<pin name="38" direction="pas" function="dot"/>
<pin name="39" direction="pas" function="dot"/>
<pin name="40" direction="pas" function="dot"/>
<pin name="41" direction="pas" function="dot"/>
<pin name="42" direction="pas" function="dot"/>
</symbol>
<symbol name="PINH2X06">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
<pin name="4" direction="pas" function="dot"/>
<pin name="5" direction="pas" function="dot"/>
<pin name="6" direction="pas" function="dot"/>
<pin name="7" direction="pas" function="dot"/>
<pin name="8" direction="pas" function="dot"/>
<pin name="9" direction="pas" function="dot"/>
<pin name="10" direction="pas" function="dot"/>
<pin name="11" direction="pas" function="dot"/>
<pin name="12" direction="pas" function="dot"/>
</symbol>
<symbol name="PINH2X13">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
<pin name="4" direction="pas" function="dot"/>
<pin name="5" direction="pas" function="dot"/>
<pin name="6" direction="pas" function="dot"/>
<pin name="7" direction="pas" function="dot"/>
<pin name="8" direction="pas" function="dot"/>
<pin name="9" direction="pas" function="dot"/>
<pin name="10" direction="pas" function="dot"/>
<pin name="11" direction="pas" function="dot"/>
<pin name="12" direction="pas" function="dot"/>
<pin name="13" direction="pas" function="dot"/>
<pin name="14" direction="pas" function="dot"/>
<pin name="15" direction="pas" function="dot"/>
<pin name="16" direction="pas" function="dot"/>
<pin name="17" direction="pas" function="dot"/>
<pin name="18" direction="pas" function="dot"/>
<pin name="19" direction="pas" function="dot"/>
<pin name="20" direction="pas" function="dot"/>
<pin name="21" direction="pas" function="dot"/>
<pin name="22" direction="pas" function="dot"/>
<pin name="23" direction="pas" function="dot"/>
<pin name="24" direction="pas" function="dot"/>
<pin name="25" direction="pas" function="dot"/>
<pin name="26" direction="pas" function="dot"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="PINHD-2X21" prefix="JP">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="PINH2X21"/>
</gates>
<devices>
<device name="_2.54" package="2X21">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="10" pad="10"/>
<connect gate="A" pin="11" pad="11"/>
<connect gate="A" pin="12" pad="12"/>
<connect gate="A" pin="13" pad="13"/>
<connect gate="A" pin="14" pad="14"/>
<connect gate="A" pin="15" pad="15"/>
<connect gate="A" pin="16" pad="16"/>
<connect gate="A" pin="17" pad="17"/>
<connect gate="A" pin="18" pad="18"/>
<connect gate="A" pin="19" pad="19"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="20" pad="20"/>
<connect gate="A" pin="21" pad="21"/>
<connect gate="A" pin="22" pad="22"/>
<connect gate="A" pin="23" pad="23"/>
<connect gate="A" pin="24" pad="24"/>
<connect gate="A" pin="25" pad="25"/>
<connect gate="A" pin="26" pad="26"/>
<connect gate="A" pin="27" pad="27"/>
<connect gate="A" pin="28" pad="28"/>
<connect gate="A" pin="29" pad="29"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="30" pad="30"/>
<connect gate="A" pin="31" pad="31"/>
<connect gate="A" pin="32" pad="32"/>
<connect gate="A" pin="33" pad="33"/>
<connect gate="A" pin="34" pad="34"/>
<connect gate="A" pin="35" pad="35"/>
<connect gate="A" pin="36" pad="36"/>
<connect gate="A" pin="37" pad="37"/>
<connect gate="A" pin="38" pad="38"/>
<connect gate="A" pin="39" pad="39"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="40" pad="40"/>
<connect gate="A" pin="41" pad="41"/>
<connect gate="A" pin="42" pad="42"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
<connect gate="A" pin="7" pad="7"/>
<connect gate="A" pin="8" pad="8"/>
<connect gate="A" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_2.54-90°" package="2X21/90">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="10" pad="10"/>
<connect gate="A" pin="11" pad="11"/>
<connect gate="A" pin="12" pad="12"/>
<connect gate="A" pin="13" pad="13"/>
<connect gate="A" pin="14" pad="14"/>
<connect gate="A" pin="15" pad="15"/>
<connect gate="A" pin="16" pad="16"/>
<connect gate="A" pin="17" pad="17"/>
<connect gate="A" pin="18" pad="18"/>
<connect gate="A" pin="19" pad="19"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="20" pad="20"/>
<connect gate="A" pin="21" pad="21"/>
<connect gate="A" pin="22" pad="22"/>
<connect gate="A" pin="23" pad="23"/>
<connect gate="A" pin="24" pad="24"/>
<connect gate="A" pin="25" pad="25"/>
<connect gate="A" pin="26" pad="26"/>
<connect gate="A" pin="27" pad="27"/>
<connect gate="A" pin="28" pad="28"/>
<connect gate="A" pin="29" pad="29"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="30" pad="30"/>
<connect gate="A" pin="31" pad="31"/>
<connect gate="A" pin="32" pad="32"/>
<connect gate="A" pin="33" pad="33"/>
<connect gate="A" pin="34" pad="34"/>
<connect gate="A" pin="35" pad="35"/>
<connect gate="A" pin="36" pad="36"/>
<connect gate="A" pin="37" pad="37"/>
<connect gate="A" pin="38" pad="38"/>
<connect gate="A" pin="39" pad="39"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="40" pad="40"/>
<connect gate="A" pin="41" pad="41"/>
<connect gate="A" pin="42" pad="42"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
<connect gate="A" pin="7" pad="7"/>
<connect gate="A" pin="8" pad="8"/>
<connect gate="A" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_2.00" package="2X21M">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="10" pad="10"/>
<connect gate="A" pin="11" pad="11"/>
<connect gate="A" pin="12" pad="12"/>
<connect gate="A" pin="13" pad="13"/>
<connect gate="A" pin="14" pad="14"/>
<connect gate="A" pin="15" pad="15"/>
<connect gate="A" pin="16" pad="16"/>
<connect gate="A" pin="17" pad="17"/>
<connect gate="A" pin="18" pad="18"/>
<connect gate="A" pin="19" pad="19"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="20" pad="20"/>
<connect gate="A" pin="21" pad="21"/>
<connect gate="A" pin="22" pad="22"/>
<connect gate="A" pin="23" pad="23"/>
<connect gate="A" pin="24" pad="24"/>
<connect gate="A" pin="25" pad="25"/>
<connect gate="A" pin="26" pad="26"/>
<connect gate="A" pin="27" pad="27"/>
<connect gate="A" pin="28" pad="28"/>
<connect gate="A" pin="29" pad="29"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="30" pad="30"/>
<connect gate="A" pin="31" pad="31"/>
<connect gate="A" pin="32" pad="32"/>
<connect gate="A" pin="33" pad="33"/>
<connect gate="A" pin="34" pad="34"/>
<connect gate="A" pin="35" pad="35"/>
<connect gate="A" pin="36" pad="36"/>
<connect gate="A" pin="37" pad="37"/>
<connect gate="A" pin="38" pad="38"/>
<connect gate="A" pin="39" pad="39"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="40" pad="40"/>
<connect gate="A" pin="41" pad="41"/>
<connect gate="A" pin="42" pad="42"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
<connect gate="A" pin="7" pad="7"/>
<connect gate="A" pin="8" pad="8"/>
<connect gate="A" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_2.54-SMD" package="2X21SMD">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="10" pad="10"/>
<connect gate="A" pin="11" pad="11"/>
<connect gate="A" pin="12" pad="12"/>
<connect gate="A" pin="13" pad="13"/>
<connect gate="A" pin="14" pad="14"/>
<connect gate="A" pin="15" pad="15"/>
<connect gate="A" pin="16" pad="16"/>
<connect gate="A" pin="17" pad="17"/>
<connect gate="A" pin="18" pad="18"/>
<connect gate="A" pin="19" pad="19"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="20" pad="20"/>
<connect gate="A" pin="21" pad="21"/>
<connect gate="A" pin="22" pad="22"/>
<connect gate="A" pin="23" pad="23"/>
<connect gate="A" pin="24" pad="24"/>
<connect gate="A" pin="25" pad="25"/>
<connect gate="A" pin="26" pad="26"/>
<connect gate="A" pin="27" pad="27"/>
<connect gate="A" pin="28" pad="28"/>
<connect gate="A" pin="29" pad="29"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="30" pad="30"/>
<connect gate="A" pin="31" pad="31"/>
<connect gate="A" pin="32" pad="32"/>
<connect gate="A" pin="33" pad="33"/>
<connect gate="A" pin="34" pad="34"/>
<connect gate="A" pin="35" pad="35"/>
<connect gate="A" pin="36" pad="36"/>
<connect gate="A" pin="37" pad="37"/>
<connect gate="A" pin="38" pad="38"/>
<connect gate="A" pin="39" pad="39"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="40" pad="40"/>
<connect gate="A" pin="41" pad="41"/>
<connect gate="A" pin="42" pad="42"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
<connect gate="A" pin="7" pad="7"/>
<connect gate="A" pin="8" pad="8"/>
<connect gate="A" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_2.54-SMD-90°" package="2X21SMD/90">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="10" pad="10"/>
<connect gate="A" pin="11" pad="11"/>
<connect gate="A" pin="12" pad="12"/>
<connect gate="A" pin="13" pad="13"/>
<connect gate="A" pin="14" pad="14"/>
<connect gate="A" pin="15" pad="15"/>
<connect gate="A" pin="16" pad="16"/>
<connect gate="A" pin="17" pad="17"/>
<connect gate="A" pin="18" pad="18"/>
<connect gate="A" pin="19" pad="19"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="20" pad="20"/>
<connect gate="A" pin="21" pad="21"/>
<connect gate="A" pin="22" pad="22"/>
<connect gate="A" pin="23" pad="23"/>
<connect gate="A" pin="24" pad="24"/>
<connect gate="A" pin="25" pad="25"/>
<connect gate="A" pin="26" pad="26"/>
<connect gate="A" pin="27" pad="27"/>
<connect gate="A" pin="28" pad="28"/>
<connect gate="A" pin="29" pad="29"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="30" pad="30"/>
<connect gate="A" pin="31" pad="31"/>
<connect gate="A" pin="32" pad="32"/>
<connect gate="A" pin="33" pad="33"/>
<connect gate="A" pin="34" pad="34"/>
<connect gate="A" pin="35" pad="35"/>
<connect gate="A" pin="36" pad="36"/>
<connect gate="A" pin="37" pad="37"/>
<connect gate="A" pin="38" pad="38"/>
<connect gate="A" pin="39" pad="39"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="40" pad="40"/>
<connect gate="A" pin="41" pad="41"/>
<connect gate="A" pin="42" pad="42"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
<connect gate="A" pin="7" pad="7"/>
<connect gate="A" pin="8" pad="8"/>
<connect gate="A" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PINHD-2X06" prefix="JP" uservalue="yes">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="PINH2X06"/>
</gates>
<devices>
<device name="_2.54" package="2X06">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="10" pad="10"/>
<connect gate="A" pin="11" pad="11"/>
<connect gate="A" pin="12" pad="12"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
<connect gate="A" pin="7" pad="7"/>
<connect gate="A" pin="8" pad="8"/>
<connect gate="A" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_2.54-90°" package="2X06/90">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="10" pad="10"/>
<connect gate="A" pin="11" pad="11"/>
<connect gate="A" pin="12" pad="12"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
<connect gate="A" pin="7" pad="7"/>
<connect gate="A" pin="8" pad="8"/>
<connect gate="A" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_2.00" package="2X06M">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="10" pad="10"/>
<connect gate="A" pin="11" pad="11"/>
<connect gate="A" pin="12" pad="12"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
<connect gate="A" pin="7" pad="7"/>
<connect gate="A" pin="8" pad="8"/>
<connect gate="A" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_2.54-SMD" package="2X06SMD">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="10" pad="10"/>
<connect gate="A" pin="11" pad="11"/>
<connect gate="A" pin="12" pad="12"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
<connect gate="A" pin="7" pad="7"/>
<connect gate="A" pin="8" pad="8"/>
<connect gate="A" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_MICROMATCH" package="MICROMATCH-12">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="10" pad="10"/>
<connect gate="A" pin="11" pad="11"/>
<connect gate="A" pin="12" pad="12"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
<connect gate="A" pin="7" pad="7"/>
<connect gate="A" pin="8" pad="8"/>
<connect gate="A" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_2.54-SMD-90°" package="2X06SMD/90">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="10" pad="10"/>
<connect gate="A" pin="11" pad="11"/>
<connect gate="A" pin="12" pad="12"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
<connect gate="A" pin="7" pad="7"/>
<connect gate="A" pin="8" pad="8"/>
<connect gate="A" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PINHD-2X13" prefix="JP" uservalue="yes">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="PINH2X13"/>
</gates>
<devices>
<device name="_2.54" package="2X13">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="10" pad="10"/>
<connect gate="A" pin="11" pad="11"/>
<connect gate="A" pin="12" pad="12"/>
<connect gate="A" pin="13" pad="13"/>
<connect gate="A" pin="14" pad="14"/>
<connect gate="A" pin="15" pad="15"/>
<connect gate="A" pin="16" pad="16"/>
<connect gate="A" pin="17" pad="17"/>
<connect gate="A" pin="18" pad="18"/>
<connect gate="A" pin="19" pad="19"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="20" pad="20"/>
<connect gate="A" pin="21" pad="21"/>
<connect gate="A" pin="22" pad="22"/>
<connect gate="A" pin="23" pad="23"/>
<connect gate="A" pin="24" pad="24"/>
<connect gate="A" pin="25" pad="25"/>
<connect gate="A" pin="26" pad="26"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
<connect gate="A" pin="7" pad="7"/>
<connect gate="A" pin="8" pad="8"/>
<connect gate="A" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_2.54-90°" package="2X13/90">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="10" pad="10"/>
<connect gate="A" pin="11" pad="11"/>
<connect gate="A" pin="12" pad="12"/>
<connect gate="A" pin="13" pad="13"/>
<connect gate="A" pin="14" pad="14"/>
<connect gate="A" pin="15" pad="15"/>
<connect gate="A" pin="16" pad="16"/>
<connect gate="A" pin="17" pad="17"/>
<connect gate="A" pin="18" pad="18"/>
<connect gate="A" pin="19" pad="19"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="20" pad="20"/>
<connect gate="A" pin="21" pad="21"/>
<connect gate="A" pin="22" pad="22"/>
<connect gate="A" pin="23" pad="23"/>
<connect gate="A" pin="24" pad="24"/>
<connect gate="A" pin="25" pad="25"/>
<connect gate="A" pin="26" pad="26"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
<connect gate="A" pin="7" pad="7"/>
<connect gate="A" pin="8" pad="8"/>
<connect gate="A" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_2.00" package="2X13M">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="10" pad="10"/>
<connect gate="A" pin="11" pad="11"/>
<connect gate="A" pin="12" pad="12"/>
<connect gate="A" pin="13" pad="13"/>
<connect gate="A" pin="14" pad="14"/>
<connect gate="A" pin="15" pad="15"/>
<connect gate="A" pin="16" pad="16"/>
<connect gate="A" pin="17" pad="17"/>
<connect gate="A" pin="18" pad="18"/>
<connect gate="A" pin="19" pad="19"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="20" pad="20"/>
<connect gate="A" pin="21" pad="21"/>
<connect gate="A" pin="22" pad="22"/>
<connect gate="A" pin="23" pad="23"/>
<connect gate="A" pin="24" pad="24"/>
<connect gate="A" pin="25" pad="25"/>
<connect gate="A" pin="26" pad="26"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
<connect gate="A" pin="7" pad="7"/>
<connect gate="A" pin="8" pad="8"/>
<connect gate="A" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_2.54-SMD" package="2X13SMD">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="10" pad="10"/>
<connect gate="A" pin="11" pad="11"/>
<connect gate="A" pin="12" pad="12"/>
<connect gate="A" pin="13" pad="13"/>
<connect gate="A" pin="14" pad="14"/>
<connect gate="A" pin="15" pad="15"/>
<connect gate="A" pin="16" pad="16"/>
<connect gate="A" pin="17" pad="17"/>
<connect gate="A" pin="18" pad="18"/>
<connect gate="A" pin="19" pad="19"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="20" pad="20"/>
<connect gate="A" pin="21" pad="21"/>
<connect gate="A" pin="22" pad="22"/>
<connect gate="A" pin="23" pad="23"/>
<connect gate="A" pin="24" pad="24"/>
<connect gate="A" pin="25" pad="25"/>
<connect gate="A" pin="26" pad="26"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
<connect gate="A" pin="7" pad="7"/>
<connect gate="A" pin="8" pad="8"/>
<connect gate="A" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="" package="2X13SMD/90">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="10" pad="10"/>
<connect gate="A" pin="11" pad="11"/>
<connect gate="A" pin="12" pad="12"/>
<connect gate="A" pin="13" pad="13"/>
<connect gate="A" pin="14" pad="14"/>
<connect gate="A" pin="15" pad="15"/>
<connect gate="A" pin="16" pad="16"/>
<connect gate="A" pin="17" pad="17"/>
<connect gate="A" pin="18" pad="18"/>
<connect gate="A" pin="19" pad="19"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="20" pad="20"/>
<connect gate="A" pin="21" pad="21"/>
<connect gate="A" pin="22" pad="22"/>
<connect gate="A" pin="23" pad="23"/>
<connect gate="A" pin="24" pad="24"/>
<connect gate="A" pin="25" pad="25"/>
<connect gate="A" pin="26" pad="26"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
<connect gate="A" pin="7" pad="7"/>
<connect gate="A" pin="8" pad="8"/>
<connect gate="A" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
<library name="rc-master-smd">
<packages>
<package name="CSV-A">
<description>&lt;b&gt;SMD ELECTROLYTIC&lt;/b&gt; - Panasonic A&lt;p&gt; 
3 mm dia</description>
</package>
<package name="CSV-B">
<description>&lt;b&gt;SMD ELECTROLYTIC&lt;/b&gt; - Panasonic B&lt;p&gt; 
4 mm dia</description>
</package>
<package name="CSV-C">
<description>&lt;b&gt;SMD ELECTROLYTIC&lt;/b&gt; - Panasonic C&lt;p&gt; 
5 mm dia</description>
</package>
<package name="CSV-D">
<description>&lt;b&gt;SMD ELECTROLYTIC&lt;/b&gt; - Panasonic D&lt;p&gt; 
6.3 mm dia</description>
</package>
<package name="CSV-E/F">
<description>&lt;b&gt;SMD ELECTROLYTIC&lt;/b&gt; - Panasonic E/F&lt;p&gt; 
8 mm dia</description>
</package>
<package name="CSV-G">
<description>&lt;b&gt;SMD ELECTROLYTIC&lt;/b&gt; - Panasonic G&lt;p&gt; 
10 mm dia</description>
</package>
<package name="C3216/T">
<description>&lt;b&gt;SMD CHIP TANT&lt;/b&gt;&lt;p&gt;
chip tantalum</description>
</package>
<package name="C3216-18/T">
<description>&lt;b&gt;SMD CHIP TANT&lt;/b&gt; - KEMET A / EIA 3216-18 Reflow solder&lt;p&gt;
KEMET S / EIA 3216-12</description>
</package>
<package name="C3528/T">
<description>&lt;b&gt;SMD CHIP TANT&lt;/b&gt;&lt;p&gt;
chip tantalum</description>
</package>
<package name="C3528-21/T">
<description>&lt;b&gt;SMD CHIP TANT&lt;/b&gt; - KEMET B / EIA 3528-21 Reflow solder&lt;p&gt;
KEMET T / EIA 3528-12</description>
</package>
<package name="C6032/T">
<description>&lt;b&gt;SMD CHIP TANT&lt;/b&gt;&lt;p&gt;
chip tantalum</description>
</package>
<package name="C6032-28/T">
<description>&lt;b&gt;SMD CHIP TANT&lt;/b&gt; - KEMET C / EIA 6032-28 Reflow solder&lt;p&gt;
KEMET U / EIA 6032-15</description>
</package>
<package name="C7343/T">
<description>&lt;b&gt;SMD CHIP TANT&lt;/b&gt;&lt;p&gt;
chip tantalum</description>
</package>
<package name="CSV-H">
<description>&lt;b&gt;SMD ELECTROLYTIC&lt;/b&gt; - Panasonic H&lt;p&gt; 
12.5 mm dia</description>
</package>
<package name="CSV-J">
<description>&lt;b&gt;SMD ELECTROLYTIC&lt;/b&gt; - Panasonic J&lt;p&gt; 
16 mm dia</description>
</package>
<package name="CSV-K">
<description>&lt;b&gt;SMD ELECTROLYTIC&lt;/b&gt; - Panasonic K&lt;p&gt; 
18 mm dia</description>
</package>
</packages>
<symbols>
<symbol name="CP-">
<pin name="-" direction="pas"/>
<pin name="+" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="CP_" prefix="C" uservalue="yes">
<description>&lt;B&gt;POLARIZED CAP&lt;/B&gt;</description>
<gates>
<gate name="G$1" symbol="CP-"/>
</gates>
<devices>
<device name="SV-A" package="CSV-A">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SV-B" package="CSV-B">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SV-C" package="CSV-C">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SV-D" package="CSV-D">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SV-E/F" package="CSV-E/F">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SV-G" package="CSV-G">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="3216" package="C3216/T">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="3216-18" package="C3216-18/T">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="3528" package="C3528/T">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="3528-21" package="C3528-21/T">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="6032" package="C6032/T">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="6032-28" package="C6032-28/T">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="7343" package="C7343/T">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SV-H" package="CSV-H">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SV-J" package="CSV-J">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SV-K" package="CSV-K">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
<library name="atmel">
<packages>
<package name="MLF64">
<description>&lt;b&gt;64M1&lt;/b&gt; Micro Lead Frame package (MLF)</description>
</package>
<package name="TQFP64">
<description>&lt;B&gt;Thin Plasic Quad Flat Package&lt;/B&gt;&lt;p&gt;
Updated from atml.lbr 17.01.2005 alf@cadsoft.de</description>
</package>
</packages>
<symbols>
<symbol name="MEGA64">
<pin name="PF0(ADC0)" direction="in"/>
<pin name="PF1(ADC1)" direction="in"/>
<pin name="PF2(ADC2)" direction="in"/>
<pin name="PF3(ADC3)" direction="in"/>
<pin name="PF4(ADC4/TCK)" direction="in"/>
<pin name="PF5(ADC5/TMS)" direction="in"/>
<pin name="PF6(ADC6/TDO)" direction="in"/>
<pin name="PF7(ADC7/TDI)" direction="in"/>
<pin name="(RXD/PDI)PE0"/>
<pin name="(TXD/PDO)PE1"/>
<pin name="(XCK0/AIN0)PE2"/>
<pin name="(OC3A/AIN1)PE3"/>
<pin name="(OC3B/INT4)PE4"/>
<pin name="(OC3C/INT5)PE5"/>
<pin name="(T3/INT6)PE6"/>
<pin name="(IC3/INT7)PE7"/>
<pin name="(T2)PD7"/>
<pin name="(T1)PD6"/>
<pin name="(XCK1)PD5"/>
<pin name="(IC1)PD4"/>
<pin name="(TXD1/INT3)PD3"/>
<pin name="(RXD1/INT2)PD2"/>
<pin name="(SDA/INT1)PD1"/>
<pin name="(SCL/INT0)PD0"/>
<pin name="(A15)PC7" direction="out"/>
<pin name="(A14)PC6" direction="out"/>
<pin name="(A13)PC5" direction="out"/>
<pin name="(A12)PC4" direction="out"/>
<pin name="(A11)PC3" direction="out"/>
<pin name="(A10)PC2" direction="out"/>
<pin name="(A9)PC1" direction="out"/>
<pin name="(A8)PC0" direction="out"/>
<pin name="(OC2/OC1C)PB7"/>
<pin name="(OC1B)PB6"/>
<pin name="(OC1A)PB5"/>
<pin name="(OC0)PB4"/>
<pin name="(MISO)PB3"/>
<pin name="(MOSI)PB2"/>
<pin name="(SCK)PB1"/>
<pin name="(SS)PB0"/>
<pin name="(AD6)PA6"/>
<pin name="(AD7)PA7"/>
<pin name="(AD5)PA5"/>
<pin name="(AD4)PA4"/>
<pin name="(AD3)PA3"/>
<pin name="(AD2)PA2"/>
<pin name="(AD1)PA1"/>
<pin name="(AD0)PA0"/>
<pin name="AVCC" direction="pwr"/>
<pin name="AGND" direction="pwr"/>
<pin name="AREF" direction="pas"/>
<pin name="XTAL1"/>
<pin name="XTAL2"/>
<pin name="VCC1" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND1" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="PG3(TOSC2)"/>
<pin name="PG4(TOSC1)"/>
<pin name="PG0(WR)" function="dot"/>
<pin name="PG1(RD)" function="dot"/>
<pin name="PG2(ALE)"/>
<pin name="RESET" direction="in" function="dot"/>
<pin name="PEN" direction="in" function="dot"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="MEGA64" prefix="IC">
<description>&lt;b&gt;MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
64 Kbytes FLASH&lt;br&gt;
4 Kbytes SRAM&lt;br&gt;
2 Kbytes EEPROM&lt;br&gt;
DUAL USART&lt;br&gt;
8-channel 10 bit ADC&lt;p&gt;
Source: avr.lbr</description>
<gates>
<gate name="G$1" symbol="MEGA64"/>
</gates>
<devices>
<device name="-M" package="MLF64">
<connects>
<connect gate="G$1" pin="(A10)PC2" pad="37"/>
<connect gate="G$1" pin="(A11)PC3" pad="38"/>
<connect gate="G$1" pin="(A12)PC4" pad="39"/>
<connect gate="G$1" pin="(A13)PC5" pad="40"/>
<connect gate="G$1" pin="(A14)PC6" pad="41"/>
<connect gate="G$1" pin="(A15)PC7" pad="42"/>
<connect gate="G$1" pin="(A8)PC0" pad="35"/>
<connect gate="G$1" pin="(A9)PC1" pad="36"/>
<connect gate="G$1" pin="(AD0)PA0" pad="51"/>
<connect gate="G$1" pin="(AD1)PA1" pad="50"/>
<connect gate="G$1" pin="(AD2)PA2" pad="49"/>
<connect gate="G$1" pin="(AD3)PA3" pad="48"/>
<connect gate="G$1" pin="(AD4)PA4" pad="47"/>
<connect gate="G$1" pin="(AD5)PA5" pad="46"/>
<connect gate="G$1" pin="(AD6)PA6" pad="45"/>
<connect gate="G$1" pin="(AD7)PA7" pad="44"/>
<connect gate="G$1" pin="(IC1)PD4" pad="29"/>
<connect gate="G$1" pin="(IC3/INT7)PE7" pad="9"/>
<connect gate="G$1" pin="(MISO)PB3" pad="13"/>
<connect gate="G$1" pin="(MOSI)PB2" pad="12"/>
<connect gate="G$1" pin="(OC0)PB4" pad="14"/>
<connect gate="G$1" pin="(OC1A)PB5" pad="15"/>
<connect gate="G$1" pin="(OC1B)PB6" pad="16"/>
<connect gate="G$1" pin="(OC2/OC1C)PB7" pad="17"/>
<connect gate="G$1" pin="(OC3A/AIN1)PE3" pad="5"/>
<connect gate="G$1" pin="(OC3B/INT4)PE4" pad="6"/>
<connect gate="G$1" pin="(OC3C/INT5)PE5" pad="7"/>
<connect gate="G$1" pin="(RXD/PDI)PE0" pad="2"/>
<connect gate="G$1" pin="(RXD1/INT2)PD2" pad="27"/>
<connect gate="G$1" pin="(SCK)PB1" pad="11"/>
<connect gate="G$1" pin="(SCL/INT0)PD0" pad="25"/>
<connect gate="G$1" pin="(SDA/INT1)PD1" pad="26"/>
<connect gate="G$1" pin="(SS)PB0" pad="10"/>
<connect gate="G$1" pin="(T1)PD6" pad="31"/>
<connect gate="G$1" pin="(T2)PD7" pad="32"/>
<connect gate="G$1" pin="(T3/INT6)PE6" pad="8"/>
<connect gate="G$1" pin="(TXD/PDO)PE1" pad="3"/>
<connect gate="G$1" pin="(TXD1/INT3)PD3" pad="28"/>
<connect gate="G$1" pin="(XCK0/AIN0)PE2" pad="4"/>
<connect gate="G$1" pin="(XCK1)PD5" pad="30"/>
<connect gate="G$1" pin="AGND" pad="63"/>
<connect gate="G$1" pin="AREF" pad="62"/>
<connect gate="G$1" pin="AVCC" pad="64"/>
<connect gate="G$1" pin="GND" pad="22"/>
<connect gate="G$1" pin="GND1" pad="53"/>
<connect gate="G$1" pin="PEN" pad="1"/>
<connect gate="G$1" pin="PF0(ADC0)" pad="61"/>
<connect gate="G$1" pin="PF1(ADC1)" pad="60"/>
<connect gate="G$1" pin="PF2(ADC2)" pad="59"/>
<connect gate="G$1" pin="PF3(ADC3)" pad="58"/>
<connect gate="G$1" pin="PF4(ADC4/TCK)" pad="57"/>
<connect gate="G$1" pin="PF5(ADC5/TMS)" pad="56"/>
<connect gate="G$1" pin="PF6(ADC6/TDO)" pad="55"/>
<connect gate="G$1" pin="PF7(ADC7/TDI)" pad="54"/>
<connect gate="G$1" pin="PG0(WR)" pad="33"/>
<connect gate="G$1" pin="PG1(RD)" pad="34"/>
<connect gate="G$1" pin="PG2(ALE)" pad="43"/>
<connect gate="G$1" pin="PG3(TOSC2)" pad="18"/>
<connect gate="G$1" pin="PG4(TOSC1)" pad="19"/>
<connect gate="G$1" pin="RESET" pad="20"/>
<connect gate="G$1" pin="VCC" pad="21"/>
<connect gate="G$1" pin="VCC1" pad="52"/>
<connect gate="G$1" pin="XTAL1" pad="24"/>
<connect gate="G$1" pin="XTAL2" pad="23"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-A" package="TQFP64">
<connects>
<connect gate="G$1" pin="(A10)PC2" pad="37"/>
<connect gate="G$1" pin="(A11)PC3" pad="38"/>
<connect gate="G$1" pin="(A12)PC4" pad="39"/>
<connect gate="G$1" pin="(A13)PC5" pad="40"/>
<connect gate="G$1" pin="(A14)PC6" pad="41"/>
<connect gate="G$1" pin="(A15)PC7" pad="42"/>
<connect gate="G$1" pin="(A8)PC0" pad="35"/>
<connect gate="G$1" pin="(A9)PC1" pad="36"/>
<connect gate="G$1" pin="(AD0)PA0" pad="51"/>
<connect gate="G$1" pin="(AD1)PA1" pad="50"/>
<connect gate="G$1" pin="(AD2)PA2" pad="49"/>
<connect gate="G$1" pin="(AD3)PA3" pad="48"/>
<connect gate="G$1" pin="(AD4)PA4" pad="47"/>
<connect gate="G$1" pin="(AD5)PA5" pad="46"/>
<connect gate="G$1" pin="(AD6)PA6" pad="45"/>
<connect gate="G$1" pin="(AD7)PA7" pad="44"/>
<connect gate="G$1" pin="(IC1)PD4" pad="29"/>
<connect gate="G$1" pin="(IC3/INT7)PE7" pad="9"/>
<connect gate="G$1" pin="(MISO)PB3" pad="13"/>
<connect gate="G$1" pin="(MOSI)PB2" pad="12"/>
<connect gate="G$1" pin="(OC0)PB4" pad="14"/>
<connect gate="G$1" pin="(OC1A)PB5" pad="15"/>
<connect gate="G$1" pin="(OC1B)PB6" pad="16"/>
<connect gate="G$1" pin="(OC2/OC1C)PB7" pad="17"/>
<connect gate="G$1" pin="(OC3A/AIN1)PE3" pad="5"/>
<connect gate="G$1" pin="(OC3B/INT4)PE4" pad="6"/>
<connect gate="G$1" pin="(OC3C/INT5)PE5" pad="7"/>
<connect gate="G$1" pin="(RXD/PDI)PE0" pad="2"/>
<connect gate="G$1" pin="(RXD1/INT2)PD2" pad="27"/>
<connect gate="G$1" pin="(SCK)PB1" pad="11"/>
<connect gate="G$1" pin="(SCL/INT0)PD0" pad="25"/>
<connect gate="G$1" pin="(SDA/INT1)PD1" pad="26"/>
<connect gate="G$1" pin="(SS)PB0" pad="10"/>
<connect gate="G$1" pin="(T1)PD6" pad="31"/>
<connect gate="G$1" pin="(T2)PD7" pad="32"/>
<connect gate="G$1" pin="(T3/INT6)PE6" pad="8"/>
<connect gate="G$1" pin="(TXD/PDO)PE1" pad="3"/>
<connect gate="G$1" pin="(TXD1/INT3)PD3" pad="28"/>
<connect gate="G$1" pin="(XCK0/AIN0)PE2" pad="4"/>
<connect gate="G$1" pin="(XCK1)PD5" pad="30"/>
<connect gate="G$1" pin="AGND" pad="63"/>
<connect gate="G$1" pin="AREF" pad="62"/>
<connect gate="G$1" pin="AVCC" pad="64"/>
<connect gate="G$1" pin="GND" pad="22"/>
<connect gate="G$1" pin="GND1" pad="53"/>
<connect gate="G$1" pin="PEN" pad="1"/>
<connect gate="G$1" pin="PF0(ADC0)" pad="61"/>
<connect gate="G$1" pin="PF1(ADC1)" pad="60"/>
<connect gate="G$1" pin="PF2(ADC2)" pad="59"/>
<connect gate="G$1" pin="PF3(ADC3)" pad="58"/>
<connect gate="G$1" pin="PF4(ADC4/TCK)" pad="57"/>
<connect gate="G$1" pin="PF5(ADC5/TMS)" pad="56"/>
<connect gate="G$1" pin="PF6(ADC6/TDO)" pad="55"/>
<connect gate="G$1" pin="PF7(ADC7/TDI)" pad="54"/>
<connect gate="G$1" pin="PG0(WR)" pad="33"/>
<connect gate="G$1" pin="PG1(RD)" pad="34"/>
<connect gate="G$1" pin="PG2(ALE)" pad="43"/>
<connect gate="G$1" pin="PG3(TOSC2)" pad="18"/>
<connect gate="G$1" pin="PG4(TOSC1)" pad="19"/>
<connect gate="G$1" pin="RESET" pad="20"/>
<connect gate="G$1" pin="VCC" pad="21"/>
<connect gate="G$1" pin="VCC1" pad="52"/>
<connect gate="G$1" pin="XTAL1" pad="24"/>
<connect gate="G$1" pin="XTAL2" pad="23"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
<library name="74xx-eu">
<packages>
<package name="DIL16">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
<package name="SO16">
<description>&lt;b&gt;Small Outline package&lt;/b&gt; 150 mil</description>
</package>
<package name="LCC20">
<description>&lt;b&gt;Leadless Chip Carrier&lt;/b&gt;&lt;p&gt; Ceramic Package</description>
</package>
</packages>
<symbols>
<symbol name="74390">
<pin name="A" direction="in" function="clk"/>
<pin name="CLR" direction="in"/>
<pin name="QA" direction="out"/>
<pin name="B" direction="in" function="clk"/>
<pin name="QB" direction="out"/>
<pin name="QC" direction="out"/>
<pin name="QD" direction="out"/>
</symbol>
<symbol name="PWRN">
<pin name="GND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
</symbol>
<symbol name="74151">
<pin name="D3" direction="in"/>
<pin name="D2" direction="in"/>
<pin name="D1" direction="in"/>
<pin name="D0" direction="in"/>
<pin name="Y" direction="out"/>
<pin name="W" direction="out" function="dot"/>
<pin name="G" direction="in" function="dot"/>
<pin name="C" direction="in"/>
<pin name="B" direction="in"/>
<pin name="A" direction="in"/>
<pin name="D7" direction="in"/>
<pin name="D6" direction="in"/>
<pin name="D5" direction="in"/>
<pin name="D4" direction="in"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="74*390" prefix="IC">
<description>Dual 4-bit decade and binary &lt;b&gt;COUNTER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="74390"/>
<gate name="B" symbol="74390"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="A" pin="A" pad="1"/>
<connect gate="A" pin="B" pad="4"/>
<connect gate="A" pin="CLR" pad="2"/>
<connect gate="A" pin="QA" pad="3"/>
<connect gate="A" pin="QB" pad="5"/>
<connect gate="A" pin="QC" pad="6"/>
<connect gate="A" pin="QD" pad="7"/>
<connect gate="B" pin="A" pad="15"/>
<connect gate="B" pin="B" pad="12"/>
<connect gate="B" pin="CLR" pad="14"/>
<connect gate="B" pin="QA" pad="13"/>
<connect gate="B" pin="QB" pad="11"/>
<connect gate="B" pin="QC" pad="10"/>
<connect gate="B" pin="QD" pad="9"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name="AC"/>
<technology name="HC"/>
<technology name="HCT"/>
<technology name="LS"/>
</technologies>
</device>
<device name="D" package="SO16">
<connects>
<connect gate="A" pin="A" pad="1"/>
<connect gate="A" pin="B" pad="4"/>
<connect gate="A" pin="CLR" pad="2"/>
<connect gate="A" pin="QA" pad="3"/>
<connect gate="A" pin="QB" pad="5"/>
<connect gate="A" pin="QC" pad="6"/>
<connect gate="A" pin="QD" pad="7"/>
<connect gate="B" pin="A" pad="15"/>
<connect gate="B" pin="B" pad="12"/>
<connect gate="B" pin="CLR" pad="14"/>
<connect gate="B" pin="QA" pad="13"/>
<connect gate="B" pin="QB" pad="11"/>
<connect gate="B" pin="QC" pad="10"/>
<connect gate="B" pin="QD" pad="9"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name="AC"/>
<technology name="HC"/>
<technology name="HCT"/>
</technologies>
</device>
<device name="FK" package="LCC20">
<connects>
<connect gate="A" pin="A" pad="2"/>
<connect gate="A" pin="B" pad="5"/>
<connect gate="A" pin="CLR" pad="3"/>
<connect gate="A" pin="QA" pad="4"/>
<connect gate="A" pin="QB" pad="7"/>
<connect gate="A" pin="QC" pad="8"/>
<connect gate="A" pin="QD" pad="9"/>
<connect gate="B" pin="A" pad="19"/>
<connect gate="B" pin="B" pad="15"/>
<connect gate="B" pin="CLR" pad="18"/>
<connect gate="B" pin="QA" pad="17"/>
<connect gate="B" pin="QB" pad="14"/>
<connect gate="B" pin="QC" pad="13"/>
<connect gate="B" pin="QD" pad="12"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="AC"/>
<technology name="HC"/>
<technology name="HCT"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*151" prefix="IC">
<description>Data &lt;b&gt;SELECTOR/MULTIPLEXER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="74151"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="A" pin="A" pad="11"/>
<connect gate="A" pin="B" pad="10"/>
<connect gate="A" pin="C" pad="9"/>
<connect gate="A" pin="D0" pad="4"/>
<connect gate="A" pin="D1" pad="3"/>
<connect gate="A" pin="D2" pad="2"/>
<connect gate="A" pin="D3" pad="1"/>
<connect gate="A" pin="D4" pad="15"/>
<connect gate="A" pin="D5" pad="14"/>
<connect gate="A" pin="D6" pad="13"/>
<connect gate="A" pin="D7" pad="12"/>
<connect gate="A" pin="G" pad="7"/>
<connect gate="A" pin="W" pad="6"/>
<connect gate="A" pin="Y" pad="5"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name=""/>
<technology name="AC"/>
<technology name="ACT"/>
<technology name="HC"/>
<technology name="HCT"/>
<technology name="LS"/>
<technology name="S"/>
</technologies>
</device>
<device name="D" package="SO16">
<connects>
<connect gate="A" pin="A" pad="11"/>
<connect gate="A" pin="B" pad="10"/>
<connect gate="A" pin="C" pad="9"/>
<connect gate="A" pin="D0" pad="4"/>
<connect gate="A" pin="D1" pad="3"/>
<connect gate="A" pin="D2" pad="2"/>
<connect gate="A" pin="D3" pad="1"/>
<connect gate="A" pin="D4" pad="15"/>
<connect gate="A" pin="D5" pad="14"/>
<connect gate="A" pin="D6" pad="13"/>
<connect gate="A" pin="D7" pad="12"/>
<connect gate="A" pin="G" pad="7"/>
<connect gate="A" pin="W" pad="6"/>
<connect gate="A" pin="Y" pad="5"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name=""/>
<technology name="AC"/>
<technology name="ACT"/>
<technology name="HC"/>
<technology name="HCT"/>
<technology name="LS"/>
<technology name="S"/>
</technologies>
</device>
<device name="FK" package="LCC20">
<connects>
<connect gate="A" pin="A" pad="14"/>
<connect gate="A" pin="B" pad="13"/>
<connect gate="A" pin="C" pad="12"/>
<connect gate="A" pin="D0" pad="5"/>
<connect gate="A" pin="D1" pad="4"/>
<connect gate="A" pin="D2" pad="3"/>
<connect gate="A" pin="D3" pad="2"/>
<connect gate="A" pin="D4" pad="19"/>
<connect gate="A" pin="D5" pad="18"/>
<connect gate="A" pin="D6" pad="17"/>
<connect gate="A" pin="D7" pad="15"/>
<connect gate="A" pin="G" pad="9"/>
<connect gate="A" pin="W" pad="8"/>
<connect gate="A" pin="Y" pad="7"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name=""/>
<technology name="AC"/>
<technology name="ACT"/>
<technology name="HC"/>
<technology name="HCT"/>
<technology name="LS"/>
<technology name="S"/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
<library name="crystal">
<description>&lt;b&gt;Crystals and Crystal Resonators&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SM77H">
<description>&lt;b&gt;3.3V CMOS Clock Oscillator&lt;/b&gt;&lt;p&gt;
Source: www.pletronics.com .. sm77h%203.3v.pdf</description>
</package>
</packages>
<symbols>
<symbol name="SM77H">
<pin name="E/D" direction="in"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="OUT" direction="out"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="SM77H" prefix="QG">
<description>&lt;b&gt;3.3V CMOS Clock Oscillator&lt;/b&gt;&lt;p&gt;
Source: www.pletronics.com .. sm77h%203.3v.pdf</description>
<gates>
<gate name="G$1" symbol="SM77H"/>
</gates>
<devices>
<device name="" package="SM77H">
<connects>
<connect gate="G$1" pin="E/D" pad="1"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="OUT" pad="3"/>
<connect gate="G$1" pin="VCC" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
<library name="pot">
<description>&lt;b&gt;Potentiometers&lt;/b&gt;&lt;p&gt;
Beckman, Copal, Piher, Spectrol, Schukat&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="B25P">
<description>&lt;b&gt;POTENTIOMETER&lt;/b&gt;&lt;p&gt;
Beckman Helitrim 25</description>
</package>
<package name="B25U">
<description>&lt;b&gt;POTENTIOMETER&lt;/b&gt;&lt;p&gt;
Beckman Helitrim 25</description>
</package>
<package name="B25V">
<description>&lt;b&gt;POTENTIOMETER&lt;/b&gt;&lt;p&gt;
Beckman Helitrim 25</description>
</package>
<package name="B25X">
<description>&lt;b&gt;POTENTIOMETER&lt;/b&gt;&lt;p&gt;
Beckman Helitrim 25</description>
</package>
<package name="B64W">
<description>&lt;b&gt;POTENTIOMETER&lt;/b&gt;&lt;p&gt;
Beckman Helitrim 64</description>
</package>
<package name="B64Y">
<description>&lt;b&gt;POTENTIOMETER&lt;/b&gt;&lt;p&gt;
Beckman Helitrim 64</description>
</package>
<package name="SP19L">
<description>&lt;b&gt;POTENTIOMETER&lt;/b&gt;</description>
</package>
<package name="CA6H">
<description>&lt;b&gt;POTENTIOMETER&lt;/b&gt;&lt;p&gt;
distributor Schukat</description>
</package>
<package name="CA6V">
<description>&lt;b&gt;POTENTIOMETER&lt;/b&gt;&lt;p&gt;
distributor Schukat</description>
</package>
<package name="CA9H">
<description>&lt;b&gt;POTENTIOMETER&lt;/b&gt;&lt;p&gt;
distributor Schukat</description>
</package>
<package name="CA9V">
<description>&lt;b&gt;POTENTIOMETER&lt;/b&gt;&lt;p&gt;
distributor Schukat</description>
</package>
<package name="CA14V">
<description>&lt;b&gt;POTENTIOMETER&lt;/b&gt;&lt;p&gt;
distributor Schukat</description>
</package>
<package name="CA14H">
<description>&lt;b&gt;POTENTIOMETER&lt;/b&gt;&lt;p&gt;
distributor Schukat</description>
</package>
<package name="CT6">
<description>&lt;b&gt;POTENTIOMETER&lt;/b&gt;&lt;p&gt;
Copal</description>
</package>
<package name="ECP10P">
<description>&lt;b&gt;POTENTIOMETER&lt;/b&gt;</description>
</package>
<package name="ECP10S">
<description>&lt;b&gt;POTENTIOMETER&lt;/b&gt;</description>
</package>
<package name="LI10">
<description>&lt;b&gt;POTENTIOMETER&lt;/b&gt;&lt;p&gt;
Piher</description>
</package>
<package name="LI15">
<description>&lt;b&gt;POTENTIOMETER&lt;/b&gt;&lt;p&gt;
Piher</description>
</package>
<package name="RJ6">
<description>&lt;b&gt;POTENTIOMETER&lt;/b&gt;&lt;p&gt;
Copal</description>
</package>
<package name="RJ6S">
<description>&lt;b&gt;POTENTIOMETER&lt;/b&gt;&lt;p&gt;
Copal</description>
</package>
<package name="RJ9W">
<description>&lt;b&gt;POTENTIOMETER&lt;/b&gt;&lt;p&gt;
Copal</description>
</package>
<package name="RS3">
<description>&lt;b&gt;POTENTIOMETER&lt;/b&gt;&lt;p&gt;
Copal</description>
</package>
<package name="S63P">
<description>&lt;b&gt;POTENTIOMETER&lt;/b&gt;&lt;p&gt;
Spectrol</description>
</package>
<package name="S63S">
<description>&lt;b&gt;POTENTIOMETER&lt;/b&gt;&lt;p&gt;
Spectrol</description>
</package>
<package name="S63X">
<description>&lt;b&gt;POTENTIOMETER&lt;/b&gt;&lt;p&gt;
Spectrol</description>
</package>
<package name="S64W">
<description>&lt;b&gt;POTENTIOMETER&lt;/b&gt;&lt;p&gt;
Spectrol</description>
</package>
<package name="S64Y">
<description>&lt;b&gt;POTENTIOMETER&lt;/b&gt;&lt;p&gt;
Spectrol</description>
</package>
<package name="S75H">
<description>&lt;b&gt;POTENTIOMETER&lt;/b&gt;</description>
</package>
<package name="S75P">
<description>&lt;b&gt;POTENTIOMETER&lt;/b&gt;</description>
</package>
<package name="ST10">
<description>&lt;b&gt;POTENTIOMETER&lt;/b&gt;&lt;p&gt;
Piher</description>
</package>
<package name="ST15">
<description>&lt;b&gt;POTENTIOMETER&lt;/b&gt;&lt;p&gt;
Piher</description>
</package>
<package name="SP19LKN">
<description>&lt;b&gt;POTENTIOMETER&lt;/b&gt;</description>
</package>
<package name="PT-10">
<description>&lt;b&gt;POTENTIOMETER&lt;/b&gt;</description>
</package>
<package name="PT-10S">
<description>&lt;b&gt;POTENTIOMETER&lt;/b&gt;</description>
</package>
<package name="PT-SPIN">
<description>&lt;b&gt;POTENTIOMETER&lt;/b&gt;</description>
</package>
<package name="CIP20C-4MM">
<description>&lt;b&gt;Carbon Rotary Potentiometers - 20 mm size&lt;/b&gt;&lt;p&gt;
Source: Radiohm .. RAD.pdf</description>
</package>
<package name="CIP20C-6MM">
<description>&lt;b&gt;Carbon Rotary Potentiometers - 20 mm size&lt;/b&gt;&lt;p&gt;
Source: Radiohm .. RAD.pdf</description>
</package>
<package name="SM-42/43A">
<description>&lt;b&gt;COPAL ELECTRONICS SM-42/43 SURFACE MOUNT TRIMMERS&lt;/b&gt; Side adjustmet&lt;p&gt;
Source: smt-pots.pdf</description>
</package>
<package name="SM-42/43B">
<description>&lt;b&gt;COPAL ELECTRONICS SM-42/43 SURFACE MOUNT TRIMMERS&lt;/b&gt; Side adjustmet&lt;p&gt;
Source: smt-pots.pdf</description>
</package>
<package name="SM-42/43W">
<description>&lt;b&gt;COPAL ELECTRONICS SM-42/43 SURFACE MOUNT TRIMMERS&lt;/b&gt; Top adjustmet&lt;p&gt;
Source: smt-pots.pdf</description>
</package>
<package name="SM-42/43X">
<description>&lt;b&gt;COPAL ELECTRONICS SM-42/43 SURFACE MOUNT TRIMMERS&lt;/b&gt; Top adjustmet&lt;p&gt;
Source: smt-pots.pdf</description>
</package>
</packages>
<symbols>
<symbol name="TPOT">
<pin name="A" direction="pas"/>
<pin name="E" direction="pas"/>
<pin name="S" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="TRIM_EU-" prefix="R" uservalue="yes">
<description>&lt;b&gt;POTENTIOMETER&lt;/b&gt;</description>
<gates>
<gate name="1" symbol="TPOT"/>
</gates>
<devices>
<device name="B25P" package="B25P">
<connects>
<connect gate="1" pin="A" pad="A"/>
<connect gate="1" pin="E" pad="E"/>
<connect gate="1" pin="S" pad="S"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="B25U" package="B25U">
<connects>
<connect gate="1" pin="A" pad="A"/>
<connect gate="1" pin="E" pad="E"/>
<connect gate="1" pin="S" pad="S"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="B25V" package="B25V">
<connects>
<connect gate="1" pin="A" pad="A"/>
<connect gate="1" pin="E" pad="E"/>
<connect gate="1" pin="S" pad="S"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="B25X" package="B25X">
<connects>
<connect gate="1" pin="A" pad="A"/>
<connect gate="1" pin="E" pad="E"/>
<connect gate="1" pin="S" pad="S"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="B64W" package="B64W">
<connects>
<connect gate="1" pin="A" pad="A"/>
<connect gate="1" pin="E" pad="E"/>
<connect gate="1" pin="S" pad="S"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="B64Y" package="B64Y">
<connects>
<connect gate="1" pin="A" pad="A"/>
<connect gate="1" pin="E" pad="E"/>
<connect gate="1" pin="S" pad="S"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="B90P" package="SP19L">
<connects>
<connect gate="1" pin="A" pad="A"/>
<connect gate="1" pin="E" pad="E"/>
<connect gate="1" pin="S" pad="S"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="CA6H" package="CA6H">
<connects>
<connect gate="1" pin="A" pad="A"/>
<connect gate="1" pin="E" pad="E"/>
<connect gate="1" pin="S" pad="S"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="CA6V" package="CA6V">
<connects>
<connect gate="1" pin="A" pad="A"/>
<connect gate="1" pin="E" pad="E"/>
<connect gate="1" pin="S" pad="S"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="CA9H" package="CA9H">
<connects>
<connect gate="1" pin="A" pad="A"/>
<connect gate="1" pin="E" pad="E"/>
<connect gate="1" pin="S" pad="S"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="CA9V" package="CA9V">
<connects>
<connect gate="1" pin="A" pad="A"/>
<connect gate="1" pin="E" pad="E"/>
<connect gate="1" pin="S" pad="S"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="CA14V" package="CA14V">
<connects>
<connect gate="1" pin="A" pad="A"/>
<connect gate="1" pin="E" pad="E"/>
<connect gate="1" pin="S" pad="S"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="CA14H" package="CA14H">
<connects>
<connect gate="1" pin="A" pad="A"/>
<connect gate="1" pin="E" pad="E"/>
<connect gate="1" pin="S" pad="S"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="CT6" package="CT6">
<connects>
<connect gate="1" pin="A" pad="A"/>
<connect gate="1" pin="E" pad="E"/>
<connect gate="1" pin="S" pad="S"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="ECP10P" package="ECP10P">
<connects>
<connect gate="1" pin="A" pad="A"/>
<connect gate="1" pin="E" pad="E"/>
<connect gate="1" pin="S" pad="S"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="ECP10S" package="ECP10S">
<connects>
<connect gate="1" pin="A" pad="A"/>
<connect gate="1" pin="E" pad="E"/>
<connect gate="1" pin="S" pad="S"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LI10" package="LI10">
<connects>
<connect gate="1" pin="A" pad="A"/>
<connect gate="1" pin="E" pad="E"/>
<connect gate="1" pin="S" pad="S"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LI15" package="LI15">
<connects>
<connect gate="1" pin="A" pad="A"/>
<connect gate="1" pin="E" pad="E"/>
<connect gate="1" pin="S" pad="S"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="RJ6" package="RJ6">
<connects>
<connect gate="1" pin="A" pad="A"/>
<connect gate="1" pin="E" pad="E"/>
<connect gate="1" pin="S" pad="S"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="RJ6S" package="RJ6S">
<connects>
<connect gate="1" pin="A" pad="A"/>
<connect gate="1" pin="E" pad="E"/>
<connect gate="1" pin="S" pad="S"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="RJ9W" package="RJ9W">
<connects>
<connect gate="1" pin="A" pad="A"/>
<connect gate="1" pin="E" pad="E"/>
<connect gate="1" pin="S" pad="S"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="RS3" package="RS3">
<connects>
<connect gate="1" pin="A" pad="A"/>
<connect gate="1" pin="E" pad="E"/>
<connect gate="1" pin="S" pad="S"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="S43P" package="SP19L">
<connects>
<connect gate="1" pin="A" pad="A"/>
<connect gate="1" pin="E" pad="E"/>
<connect gate="1" pin="S" pad="S"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="S63P" package="S63P">
<connects>
<connect gate="1" pin="A" pad="A"/>
<connect gate="1" pin="E" pad="E"/>
<connect gate="1" pin="S" pad="S"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="S63S" package="S63S">
<connects>
<connect gate="1" pin="A" pad="A"/>
<connect gate="1" pin="E" pad="E"/>
<connect gate="1" pin="S" pad="S"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="S63X" package="S63X">
<connects>
<connect gate="1" pin="A" pad="A"/>
<connect gate="1" pin="E" pad="E"/>
<connect gate="1" pin="S" pad="S"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="S64W" package="S64W">
<connects>
<connect gate="1" pin="A" pad="A"/>
<connect gate="1" pin="E" pad="E"/>
<connect gate="1" pin="S" pad="S"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="S64Y" package="S64Y">
<connects>
<connect gate="1" pin="A" pad="A"/>
<connect gate="1" pin="E" pad="E"/>
<connect gate="1" pin="S" pad="S"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="S75H" package="S75H">
<connects>
<connect gate="1" pin="A" pad="A"/>
<connect gate="1" pin="E" pad="E"/>
<connect gate="1" pin="S" pad="S"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="S75P" package="S75P">
<connects>
<connect gate="1" pin="A" pad="A"/>
<connect gate="1" pin="E" pad="E"/>
<connect gate="1" pin="S" pad="S"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SP19L" package="SP19L">
<connects>
<connect gate="1" pin="A" pad="A"/>
<connect gate="1" pin="E" pad="E"/>
<connect gate="1" pin="S" pad="S"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="ST10" package="ST10">
<connects>
<connect gate="1" pin="A" pad="A"/>
<connect gate="1" pin="E" pad="E"/>
<connect gate="1" pin="S" pad="S"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="ST15" package="ST15">
<connects>
<connect gate="1" pin="A" pad="A"/>
<connect gate="1" pin="E" pad="E"/>
<connect gate="1" pin="S" pad="S"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="T189" package="SP19LKN">
<connects>
<connect gate="1" pin="A" pad="A"/>
<connect gate="1" pin="E" pad="E"/>
<connect gate="1" pin="S" pad="S"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PT10" package="PT-10">
<connects>
<connect gate="1" pin="A" pad="A"/>
<connect gate="1" pin="E" pad="E"/>
<connect gate="1" pin="S" pad="S"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PT10S" package="PT-10S">
<connects>
<connect gate="1" pin="A" pad="A"/>
<connect gate="1" pin="E" pad="E"/>
<connect gate="1" pin="S" pad="S"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PTSPIN" package="PT-SPIN">
<connects>
<connect gate="1" pin="A" pad="A"/>
<connect gate="1" pin="E" pad="E"/>
<connect gate="1" pin="S" pad="S"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="CIP20C-4MM" package="CIP20C-4MM">
<connects>
<connect gate="1" pin="A" pad="A"/>
<connect gate="1" pin="E" pad="E"/>
<connect gate="1" pin="S" pad="S"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="CIP20C-6MM" package="CIP20C-6MM">
<connects>
<connect gate="1" pin="A" pad="A"/>
<connect gate="1" pin="E" pad="E"/>
<connect gate="1" pin="S" pad="S"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SM-42/43A" package="SM-42/43A">
<connects>
<connect gate="1" pin="A" pad="1"/>
<connect gate="1" pin="E" pad="3"/>
<connect gate="1" pin="S" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SM-42/43B" package="SM-42/43B">
<connects>
<connect gate="1" pin="A" pad="1"/>
<connect gate="1" pin="E" pad="3"/>
<connect gate="1" pin="S" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SM-42/43W" package="SM-42/43W">
<connects>
<connect gate="1" pin="A" pad="1"/>
<connect gate="1" pin="E" pad="3"/>
<connect gate="1" pin="S" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SM-42/43X" package="SM-42/43X">
<connects>
<connect gate="1" pin="A" pad="1"/>
<connect gate="1" pin="E" pad="3"/>
<connect gate="1" pin="S" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<parts>
<part name="FRAME1" library="FRAMES" deviceset="DINA4_L" device=""/>
<part name="R7" library="1Eigene" deviceset="WIDERSTAND_10" device="" value="10k"/>
<part name="P+4" library="supply1" deviceset="+5V" device=""/>
<part name="GND12" library="supply1" deviceset="GND" device=""/>
<part name="GND3" library="supply1" deviceset="GND" device=""/>
<part name="P+2" library="supply1" deviceset="+5V" device=""/>
<part name="GND13" library="supply1" deviceset="GND" device=""/>
<part name="P+7" library="supply1" deviceset="+5V" device=""/>
<part name="R1" library="rcl" deviceset="R-EU_" device="R0805" value="2,2k"/>
<part name="R2" library="rcl" deviceset="R-EU_" device="R0805" value="1k"/>
<part name="Q2" library="transistor-npn" deviceset="BC546*" device="" technology="A"/>
<part name="GND5" library="supply1" deviceset="GND" device=""/>
<part name="GND14" library="supply1" deviceset="GND" device=""/>
<part name="GND16" library="supply1" deviceset="GND" device=""/>
<part name="C2" library="rcl" deviceset="C-EU" device="025-025X050" value="0,1µ"/>
<part name="P+3" library="supply1" deviceset="+5V" device=""/>
<part name="C3" library="rcl" deviceset="C-EU" device="C0805K" value="0,1µ"/>
<part name="SW1" library="1Eigene" deviceset="SW-PUSH-90" device="" value="Taster"/>
<part name="SW2" library="1Eigene" deviceset="SW-PUSH-90" device="" value="3305"/>
<part name="P+9" library="supply1" deviceset="+5V" device=""/>
<part name="GND2" library="supply1" deviceset="GND" device=""/>
<part name="SW3" library="1Eigene" deviceset="ESP201" device=""/>
<part name="C5" library="rcl" deviceset="C-EU" device="C0805" value="0,1µF"/>
<part name="C4" library="rc-master-smd" deviceset="CP_" device="SV-D" value="100µF"/>
<part name="IC2" library="atmel" deviceset="MEGA64" device="-A"/>
<part name="SW4" library="1Eigene" deviceset="SW-PUSH-90" device="" value="Taster 3305"/>
<part name="BOARD3" library="pinhead-2" deviceset="PINHD-2X21" device="_2.54-90°" value="zur Busplatine"/>
<part name="IC3" library="1Eigene" deviceset="LM809M3-4.63" device=""/>
<part name="R4" library="rcl" deviceset="R-EU_" device="R0805" value="1k"/>
<part name="P+6" library="supply1" deviceset="+5V" device=""/>
<part name="GND1" library="supply1" deviceset="GND" device=""/>
<part name="IC1" library="74xx-eu" deviceset="74*390" device="D" technology="HCT"/>
<part name="GND4" library="supply1" deviceset="GND" device=""/>
<part name="IC4" library="74xx-eu" deviceset="74*390" device="D" technology="HCT"/>
<part name="GND8" library="supply1" deviceset="GND" device=""/>
<part name="IC5" library="74xx-eu" deviceset="74*390" device="D" technology="HCT"/>
<part name="GND9" library="supply1" deviceset="GND" device=""/>
<part name="GND11" library="supply1" deviceset="GND" device=""/>
<part name="IC6" library="74xx-eu" deviceset="74*151" device="D" technology="S" value="74LS151D"/>
<part name="JP2" library="pinhead-2" deviceset="PINHD-2X06" device="_2.54-90°" value="ISP+JTAG"/>
<part name="QG1" library="crystal" deviceset="SM77H" device=""/>
<part name="P+1" library="supply1" deviceset="+5V" device=""/>
<part name="GND6" library="supply1" deviceset="GND" device=""/>
<part name="JP1" library="pinhead-2" deviceset="PINHD-2X13" device="_2.54-90°"/>
<part name="R5" library="pot" deviceset="TRIM_EU-" device="CA6H" value="2,5k"/>
<part name="P+8" library="supply1" deviceset="+5V" device=""/>
<part name="P+5" library="supply1" deviceset="+5V" device=""/>
<part name="GND7" library="supply1" deviceset="GND" device=""/>
<part name="C1" library="rcl" deviceset="C-EU" device="C0805" value="0,1µF"/>
<part name="R3" library="rcl" deviceset="R-EU_" device="R0805" value="1k"/>
<part name="R6" library="rcl" deviceset="R-EU_" device="R0805" value="1k"/>
</parts>
<sheets>
<sheet>
<plain>
<text>scan</text>
<text>Trigger</text>
<text>Counter für TR4111A</text>
<text>D0-D7= Daten aus Counter</text>
<text>E,RS,DB4-DB7=Display</text>
<text>SP1-SP7= Einstellung Spectrumanalyser</text>
<text>PR2-PR4= Programmierung Spectrumanalyser</text>
<text>Span1</text>
<text>Span2</text>
<text>Span3</text>
<text>Span4</text>
<text>1,5-3,5Ghz</text>
<text>2,5-4,5GHz</text>
<text>PR1= Kalibrierung</text>
<text>kalibrieren</text>
<text>speichern</text>
<text>vorwärts</text>
<text>rückwärts</text>
<text>Out</text>
<text>In</text>
<text>Poweron reset</text>
<text>1MHz</text>
<text>10KHZ</text>
<text>1KHz</text>
<text>A  B</text>
<text>0  0   2,56ms</text>
<text>1  0   25,6ms</text>
<text>0  1   256ms</text>
<text>1  1   2,56Sek</text>
<text>store</text>
<text>reset</text>
<text>Clock</text>
<text>Chip-Select</text>
<text>ISP6</text>
<text>ISP2</text>
<text>ISP4</text>
<text>ISP8</text>
<text>ISP10</text>
<text>ISP12</text>
<text>ISP_CLOCK</text>
</plain>
<busses>
<bus name="ADC[15..19]">
<segment>
</segment>
</bus>
<bus name="D[0..7]">
<segment>
</segment>
</bus>
<bus name="SP[1..10],TRIGGER,PD9">
<segment>
</segment>
</bus>
<bus name="TDI,TDO,TMS,TCK,RESET">
<segment>
</segment>
</bus>
</busses>
<nets>
<net name="GND">
<segment>
<pinref part="GND3" gate="1" pin="GND"/>
<pinref part="C3" gate="G$1" pin="2"/>
<pinref part="C5" gate="G$1" pin="1"/>
<pinref part="IC2" gate="G$1" pin="GND"/>
<pinref part="IC2" gate="G$1" pin="GND1"/>
<pinref part="IC2" gate="G$1" pin="AGND"/>
</segment>
<segment>
<pinref part="GND13" gate="1" pin="GND"/>
<pinref part="IC1" gate="P" pin="GND"/>
<pinref part="IC4" gate="P" pin="GND"/>
<pinref part="IC5" gate="P" pin="GND"/>
<pinref part="IC6" gate="P" pin="GND"/>
<pinref part="C2" gate="G$1" pin="2"/>
<pinref part="C1" gate="G$1" pin="1"/>
</segment>
<segment>
<pinref part="GND12" gate="1" pin="GND"/>
<pinref part="BOARD3" gate="A" pin="20"/>
<pinref part="BOARD3" gate="A" pin="22"/>
</segment>
<segment>
<pinref part="GND5" gate="1" pin="GND"/>
<pinref part="Q2" gate="G$1" pin="E"/>
</segment>
<segment>
<pinref part="GND14" gate="1" pin="GND"/>
<pinref part="R2" gate="G$1" pin="1"/>
<pinref part="C4" gate="G$1" pin="-"/>
<pinref part="JP1" gate="A" pin="24"/>
<pinref part="JP1" gate="A" pin="26"/>
<pinref part="JP1" gate="A" pin="23"/>
</segment>
<segment>
<pinref part="GND16" gate="1" pin="GND"/>
<pinref part="SW1" gate="G$1" pin="P1"/>
<pinref part="SW1" gate="G$1" pin="G1"/>
<pinref part="SW2" gate="G$1" pin="P1"/>
<pinref part="SW2" gate="G$1" pin="G1"/>
<pinref part="SW1" gate="G$1" pin="G2"/>
<pinref part="SW2" gate="G$1" pin="G2"/>
<pinref part="SW3" gate="G$1" pin="1"/>
<pinref part="SW4" gate="G$1" pin="P1"/>
<pinref part="SW4" gate="G$1" pin="G1"/>
<pinref part="SW4" gate="G$1" pin="G2"/>
</segment>
<segment>
<pinref part="GND2" gate="1" pin="GND"/>
<pinref part="JP2" gate="A" pin="12"/>
<pinref part="JP2" gate="A" pin="11"/>
</segment>
<segment>
<pinref part="GND1" gate="1" pin="GND"/>
<pinref part="IC3" gate="G$1" pin="GND"/>
</segment>
<segment>
<pinref part="IC1" gate="A" pin="CLR"/>
<pinref part="IC1" gate="B" pin="CLR"/>
<pinref part="GND4" gate="1" pin="GND"/>
</segment>
<segment>
<pinref part="IC4" gate="A" pin="CLR"/>
<pinref part="IC4" gate="B" pin="CLR"/>
<pinref part="GND8" gate="1" pin="GND"/>
</segment>
<segment>
<pinref part="IC5" gate="A" pin="CLR"/>
<pinref part="GND9" gate="1" pin="GND"/>
</segment>
<segment>
<pinref part="GND11" gate="1" pin="GND"/>
<pinref part="IC6" gate="A" pin="G"/>
</segment>
<segment>
<pinref part="QG1" gate="G$1" pin="GND"/>
<pinref part="GND6" gate="1" pin="GND"/>
</segment>
<segment>
<pinref part="GND7" gate="1" pin="GND"/>
<pinref part="JP1" gate="A" pin="1"/>
</segment>
</net>
<net name="+5V">
<segment>
<pinref part="R7" gate="G$1" pin="2"/>
<pinref part="P+4" gate="1" pin="+5V"/>
<pinref part="C5" gate="G$1" pin="2"/>
<pinref part="IC2" gate="G$1" pin="AVCC"/>
<pinref part="IC2" gate="G$1" pin="VCC"/>
<pinref part="IC2" gate="G$1" pin="VCC1"/>
</segment>
<segment>
<pinref part="P+9" gate="1" pin="+5V"/>
<pinref part="JP2" gate="A" pin="4"/>
</segment>
<segment>
<pinref part="P+3" gate="1" pin="+5V"/>
<pinref part="C4" gate="G$1" pin="+"/>
<pinref part="JP1" gate="A" pin="20"/>
<pinref part="JP1" gate="A" pin="22"/>
</segment>
<segment>
<pinref part="P+7" gate="1" pin="+5V"/>
<pinref part="BOARD3" gate="A" pin="18"/>
<pinref part="BOARD3" gate="A" pin="16"/>
</segment>
<segment>
<pinref part="P+6" gate="1" pin="+5V"/>
<pinref part="IC3" gate="G$1" pin="VCC"/>
</segment>
<segment>
<pinref part="P+2" gate="1" pin="+5V"/>
<pinref part="C2" gate="G$1" pin="1"/>
<pinref part="IC6" gate="P" pin="VCC"/>
<pinref part="IC5" gate="P" pin="VCC"/>
<pinref part="IC4" gate="P" pin="VCC"/>
<pinref part="IC1" gate="P" pin="VCC"/>
<pinref part="C1" gate="G$1" pin="2"/>
</segment>
<segment>
<pinref part="QG1" gate="G$1" pin="VCC"/>
<pinref part="P+1" gate="1" pin="+5V"/>
</segment>
<segment>
<pinref part="R5" gate="1" pin="E"/>
<pinref part="P+8" gate="1" pin="+5V"/>
</segment>
<segment>
<pinref part="P+5" gate="1" pin="+5V"/>
<pinref part="JP1" gate="A" pin="15"/>
</segment>
</net>
<net name="ENABLE">
<segment>
<pinref part="IC2" gate="G$1" pin="(IC1)PD4"/>
<pinref part="BOARD3" gate="A" pin="12"/>
</segment>
</net>
<net name="CNT_RESET">
<segment>
<pinref part="IC2" gate="G$1" pin="(SDA/INT1)PD1"/>
<pinref part="BOARD3" gate="A" pin="13"/>
</segment>
</net>
<net name="D0">
<segment>
<pinref part="IC2" gate="G$1" pin="(OC3B/INT4)PE4"/>
</segment>
<segment>
<pinref part="BOARD3" gate="A" pin="30"/>
</segment>
</net>
<net name="D1">
<segment>
<pinref part="IC2" gate="G$1" pin="(XCK0/AIN0)PE2"/>
</segment>
<segment>
<pinref part="BOARD3" gate="A" pin="32"/>
</segment>
</net>
<net name="D4">
<segment>
<pinref part="IC2" gate="G$1" pin="(AD0)PA0"/>
</segment>
<segment>
<pinref part="BOARD3" gate="A" pin="38"/>
</segment>
</net>
<net name="D5">
<segment>
<pinref part="IC2" gate="G$1" pin="(AD1)PA1"/>
</segment>
<segment>
<pinref part="BOARD3" gate="A" pin="40"/>
</segment>
</net>
<net name="D6">
<segment>
<pinref part="BOARD3" gate="A" pin="31"/>
</segment>
<segment>
<pinref part="IC2" gate="G$1" pin="(OC2/OC1C)PB7"/>
</segment>
</net>
<net name="D7">
<segment>
<pinref part="IC2" gate="G$1" pin="(OC3A/AIN1)PE3"/>
</segment>
<segment>
<pinref part="BOARD3" gate="A" pin="33"/>
</segment>
</net>
<net name="D2">
<segment>
<pinref part="BOARD3" gate="A" pin="34"/>
</segment>
<segment>
<pinref part="IC2" gate="G$1" pin="(OC1B)PB6"/>
</segment>
</net>
<net name="D3">
<segment>
<pinref part="IC2" gate="G$1" pin="(AD2)PA2"/>
</segment>
<segment>
<pinref part="BOARD3" gate="A" pin="36"/>
</segment>
</net>
<net name="ADC19">
<segment>
<pinref part="BOARD3" gate="A" pin="28"/>
</segment>
<segment>
<pinref part="IC2" gate="G$1" pin="(SCK)PB1"/>
<pinref part="JP2" gate="A" pin="6"/>
<pinref part="JP1" gate="A" pin="17"/>
</segment>
</net>
<net name="ADC18">
<segment>
<pinref part="R3" gate="G$1" pin="2"/>
</segment>
<segment>
<pinref part="IC2" gate="G$1" pin="(MISO)PB3"/>
</segment>
</net>
<net name="ADC16">
<segment>
<pinref part="R6" gate="G$1" pin="1"/>
</segment>
<segment>
<pinref part="IC2" gate="G$1" pin="(MOSI)PB2"/>
</segment>
</net>
<net name="ADC15">
<segment>
<pinref part="BOARD3" gate="A" pin="25"/>
</segment>
<segment>
<pinref part="IC2" gate="G$1" pin="(SS)PB0"/>
</segment>
</net>
<net name="SP3">
<segment>
<pinref part="IC2" gate="G$1" pin="(A11)PC3"/>
</segment>
<segment>
<pinref part="JP1" gate="A" pin="6"/>
</segment>
</net>
<net name="N$6">
<segment>
<pinref part="R1" gate="G$1" pin="1"/>
<pinref part="R2" gate="G$1" pin="2"/>
<pinref part="Q2" gate="G$1" pin="B"/>
</segment>
</net>
<net name="PD9">
<segment>
<pinref part="IC2" gate="G$1" pin="PF0(ADC0)"/>
</segment>
<segment>
<pinref part="R1" gate="G$1" pin="2"/>
</segment>
</net>
<net name="SWEEPHOLD">
<segment>
<pinref part="Q2" gate="G$1" pin="C"/>
<pinref part="JP1" gate="A" pin="16"/>
</segment>
</net>
<net name="CNT_STORE">
<segment>
<pinref part="IC2" gate="G$1" pin="(RXD1/INT2)PD2"/>
<pinref part="BOARD3" gate="A" pin="11"/>
</segment>
</net>
<net name="COLD">
<segment>
<pinref part="IC2" gate="G$1" pin="(AD6)PA6"/>
<pinref part="BOARD3" gate="A" pin="17"/>
</segment>
</net>
<net name="EXT">
<segment>
<pinref part="IC2" gate="G$1" pin="(AD5)PA5"/>
<pinref part="BOARD3" gate="A" pin="14"/>
</segment>
</net>
<net name="HELL">
<segment>
<pinref part="BOARD3" gate="A" pin="6"/>
<pinref part="R5" gate="1" pin="S"/>
</segment>
</net>
<net name="OSC_OFF">
<segment>
<pinref part="BOARD3" gate="A" pin="4"/>
<pinref part="IC2" gate="G$1" pin="(A14)PC6"/>
</segment>
</net>
<net name="RS">
<segment>
<pinref part="IC2" gate="G$1" pin="(AD7)PA7"/>
<pinref part="BOARD3" gate="A" pin="19"/>
</segment>
</net>
<net name="DB5">
<segment>
<pinref part="IC2" gate="G$1" pin="(AD3)PA3"/>
<pinref part="BOARD3" gate="A" pin="8"/>
</segment>
</net>
<net name="CENT">
<segment>
<pinref part="IC2" gate="G$1" pin="(AD4)PA4"/>
<pinref part="BOARD3" gate="A" pin="10"/>
</segment>
</net>
<net name="DB4">
<segment>
<pinref part="IC2" gate="G$1" pin="(OC1A)PB5"/>
<pinref part="BOARD3" gate="A" pin="5"/>
</segment>
</net>
<net name="PR3">
<segment>
<pinref part="SW2" gate="G$1" pin="S1"/>
<pinref part="IC2" gate="G$1" pin="PF1(ADC1)"/>
<pinref part="JP1" gate="A" pin="9"/>
</segment>
</net>
<net name="PR2">
<segment>
<pinref part="SW1" gate="G$1" pin="S1"/>
<pinref part="IC2" gate="G$1" pin="PF2(ADC2)"/>
<pinref part="JP1" gate="A" pin="7"/>
</segment>
</net>
<net name="PR1">
<segment>
<pinref part="SW3" gate="G$1" pin="C"/>
<pinref part="IC2" gate="G$1" pin="PF3(ADC3)"/>
<pinref part="JP1" gate="A" pin="3"/>
</segment>
</net>
<net name="PR4">
<segment>
<pinref part="IC2" gate="G$1" pin="(RXD/PDI)PE0"/>
<pinref part="SW4" gate="G$1" pin="S1"/>
<pinref part="JP2" gate="A" pin="8"/>
<pinref part="JP1" gate="A" pin="19"/>
<pinref part="JP1" gate="A" pin="5"/>
</segment>
</net>
<net name="COUNT_ENDED">
<segment>
<pinref part="IC2" gate="G$1" pin="(OC3C/INT5)PE5"/>
<pinref part="BOARD3" gate="A" pin="1"/>
</segment>
</net>
<net name="E">
<segment>
<pinref part="IC2" gate="G$1" pin="(T3/INT6)PE6"/>
<pinref part="BOARD3" gate="A" pin="3"/>
</segment>
</net>
<net name="DB7">
<segment>
<pinref part="IC2" gate="G$1" pin="(IC3/INT7)PE7"/>
<pinref part="BOARD3" gate="A" pin="2"/>
</segment>
</net>
<net name="10MHZ_IN">
<segment>
<pinref part="BOARD3" gate="A" pin="23"/>
<pinref part="IC1" gate="A" pin="B"/>
</segment>
</net>
<net name="TIME_A">
<segment>
<pinref part="IC2" gate="G$1" pin="(T2)PD7"/>
<pinref part="IC6" gate="A" pin="A"/>
</segment>
</net>
<net name="COUNTSTART">
<segment>
<pinref part="IC2" gate="G$1" pin="(XCK1)PD5"/>
<pinref part="BOARD3" gate="A" pin="21"/>
</segment>
</net>
<net name="SP6">
<segment>
<pinref part="IC2" gate="G$1" pin="(A8)PC0"/>
</segment>
<segment>
<pinref part="JP1" gate="A" pin="12"/>
</segment>
</net>
<net name="SP5">
<segment>
<pinref part="IC2" gate="G$1" pin="(A9)PC1"/>
</segment>
<segment>
<pinref part="JP1" gate="A" pin="10"/>
</segment>
</net>
<net name="SP4">
<segment>
<pinref part="IC2" gate="G$1" pin="(A10)PC2"/>
</segment>
<segment>
<pinref part="JP1" gate="A" pin="8"/>
</segment>
</net>
<net name="SP2">
<segment>
<pinref part="IC2" gate="G$1" pin="(A12)PC4"/>
</segment>
<segment>
<pinref part="JP1" gate="A" pin="4"/>
</segment>
</net>
<net name="SP1">
<segment>
<pinref part="IC2" gate="G$1" pin="(A13)PC5"/>
</segment>
<segment>
<pinref part="JP1" gate="A" pin="2"/>
</segment>
</net>
<net name="SP7">
<segment>
<pinref part="IC2" gate="G$1" pin="(A15)PC7"/>
</segment>
<segment>
<pinref part="JP1" gate="A" pin="14"/>
</segment>
</net>
<net name="N$2">
<segment>
<pinref part="IC3" gate="G$1" pin="/RESET"/>
<pinref part="R4" gate="G$1" pin="1"/>
</segment>
</net>
<net name="TIME_B">
<segment>
<pinref part="IC2" gate="G$1" pin="(T1)PD6"/>
<pinref part="IC6" gate="A" pin="B"/>
</segment>
</net>
<net name="SCAN">
<segment>
<pinref part="IC2" gate="G$1" pin="(TXD1/INT3)PD3"/>
<pinref part="BOARD3" gate="A" pin="24"/>
</segment>
</net>
<net name="1MHZ">
<segment>
<pinref part="IC1" gate="A" pin="QA"/>
<pinref part="IC1" gate="B" pin="B"/>
</segment>
</net>
<net name="100KHZ">
<segment>
<pinref part="IC6" gate="A" pin="D0"/>
<pinref part="IC1" gate="B" pin="QA"/>
<pinref part="IC4" gate="A" pin="B"/>
<pinref part="IC6" gate="A" pin="D7"/>
<pinref part="IC6" gate="A" pin="D4"/>
<pinref part="IC6" gate="A" pin="D6"/>
<pinref part="IC6" gate="A" pin="D5"/>
</segment>
</net>
<net name="10KHZ">
<segment>
<pinref part="IC6" gate="A" pin="D1"/>
<pinref part="IC4" gate="A" pin="QA"/>
<pinref part="IC4" gate="B" pin="B"/>
</segment>
</net>
<net name="CLOCK">
<segment>
<pinref part="IC6" gate="A" pin="W"/>
<pinref part="BOARD3" gate="A" pin="9"/>
</segment>
</net>
<net name="100HZ">
<segment>
<pinref part="IC6" gate="A" pin="D3"/>
<pinref part="IC5" gate="A" pin="QA"/>
</segment>
</net>
<net name="N$4">
<segment>
<pinref part="IC1" gate="A" pin="QD"/>
<pinref part="IC1" gate="A" pin="A"/>
</segment>
</net>
<net name="N$11">
<segment>
<pinref part="IC1" gate="B" pin="QD"/>
<pinref part="IC1" gate="B" pin="A"/>
</segment>
</net>
<net name="N$17">
<segment>
<pinref part="IC4" gate="A" pin="A"/>
<pinref part="IC4" gate="A" pin="QD"/>
</segment>
</net>
<net name="1KHZ">
<segment>
<pinref part="IC6" gate="A" pin="D2"/>
<pinref part="IC4" gate="B" pin="QA"/>
<pinref part="IC5" gate="A" pin="B"/>
</segment>
</net>
<net name="N$18">
<segment>
<pinref part="IC4" gate="B" pin="A"/>
<pinref part="IC4" gate="B" pin="QD"/>
</segment>
</net>
<net name="N$15">
<segment>
<pinref part="IC5" gate="A" pin="A"/>
<pinref part="IC5" gate="A" pin="QD"/>
</segment>
</net>
<net name="MPX_C">
<segment>
<pinref part="BOARD3" gate="A" pin="42"/>
<pinref part="IC6" gate="A" pin="C"/>
</segment>
</net>
<net name="DB6">
<segment>
<pinref part="BOARD3" gate="A" pin="7"/>
<pinref part="IC2" gate="G$1" pin="(TXD/PDO)PE1"/>
<pinref part="JP2" gate="A" pin="2"/>
<pinref part="JP1" gate="A" pin="13"/>
</segment>
</net>
<net name="TDI">
<segment>
<pinref part="IC2" gate="G$1" pin="PF7(ADC7/TDI)"/>
</segment>
<segment>
<pinref part="JP2" gate="A" pin="1"/>
</segment>
</net>
<net name="TDO">
<segment>
<pinref part="IC2" gate="G$1" pin="PF6(ADC6/TDO)"/>
</segment>
<segment>
<pinref part="JP2" gate="A" pin="5"/>
</segment>
</net>
<net name="TMS">
<segment>
<pinref part="IC2" gate="G$1" pin="PF5(ADC5/TMS)"/>
</segment>
<segment>
<pinref part="JP2" gate="A" pin="3"/>
</segment>
</net>
<net name="TCK">
<segment>
<pinref part="IC2" gate="G$1" pin="PF4(ADC4/TCK)"/>
</segment>
<segment>
<pinref part="JP2" gate="A" pin="7"/>
</segment>
</net>
<net name="TRIGGER">
<segment>
<pinref part="BOARD3" gate="A" pin="15"/>
</segment>
<segment>
<pinref part="IC2" gate="G$1" pin="(SCL/INT0)PD0"/>
</segment>
</net>
<net name="10MHZ_QUARZ">
<segment>
<pinref part="QG1" gate="G$1" pin="OUT"/>
<pinref part="IC2" gate="G$1" pin="XTAL1"/>
</segment>
</net>
<net name="RESET">
<segment>
<pinref part="R4" gate="G$1" pin="2"/>
<pinref part="IC2" gate="G$1" pin="RESET"/>
<pinref part="R7" gate="G$1" pin="1"/>
<pinref part="C3" gate="G$1" pin="1"/>
<pinref part="JP2" gate="A" pin="10"/>
<pinref part="JP2" gate="A" pin="9"/>
<pinref part="JP1" gate="A" pin="21"/>
</segment>
</net>
<net name="N$5">
<segment>
<pinref part="BOARD3" gate="A" pin="27"/>
<pinref part="R3" gate="G$1" pin="1"/>
</segment>
</net>
<net name="N$7">
<segment>
<pinref part="R6" gate="G$1" pin="2"/>
<pinref part="BOARD3" gate="A" pin="26"/>
</segment>
</net>
<net name="ABBRUCH">
<segment>
<pinref part="BOARD3" gate="A" pin="37"/>
<pinref part="IC2" gate="G$1" pin="(OC0)PB4"/>
</segment>
</net>
</nets>
</sheet>
</sheets>
</schematic>
</drawing>
</eagle>
